110488     RSXPROM  Version: 1.3, July 1981
 
Submitted by: Richard C. Noonan, NOVA Biomedical, Newton, MA
 
Operating System: RSX-11M V3.2  Source Language: MACRO-11  Memory
Required: 41K  Hardware Required: DATA I/O System 19 ERROM Programmer
with Computer Remote Control, second serial port.  Keywords: EPROM
 
Abstract: RSXPROM provides the capability for downloading Intel
HEX format files from an RSX-11M system to a DATA I/O
System 19 EPROM programmer (with Computer Remote
Control) via a serial line. RSXPROM reads the specified
HEX file from disk, transmits a chunk of the file
(representing 4K bytes of object code) starting at the
specified address, and sets up the Block Limits in the
DATA I/O for programming the specified type of EPROM.
RSXPROM has been used successfully with the DATA I/O
single-PROM modules for the 2708 and the 2716/2732, and
with the Gang Programming module.
 
Restrictions: File to be transmitted must fit in memory buffer. Works
only with 2708, 2716/2516, and 2732/2532 type EPROMS.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: FILES-11,
600' Magnetic Tape (MA)  Format: FILES-11
 
 
