110910     MAIL  Version: 1.14, January 1988
 
Submitted by: Mike Marak, Concordia Univ., EMC Lab., Loyola Campus,
Montreal, Quebec, Canada  H4B 1R6
 
Operating System: RT-11 V5.4, TSX-PLUS V6.2  Source Language: FORTRAN
IV  Memory Required: 32KB  Software Required: FORTRAN IV  Keywords:
Data Communications, Mail, System Management - RT-11, Utilities -
Terminal
 
Abstract: MAIL is a message handling system for use under TSX-PLUS.
It allows users registered with the mail system to read
their messages or send messages to other registered users.
The messages are stored in a file, and users can only read
messages that are sent to them.
 
The creation of the mail file and registering users is done
by the POSTMN.TSX program.
 
Messages are limited to 1000 bytes maximum, and each user
has a total of 2500 bytes of message storage.
 
Documentation is included, as well as a log of a sample
session, and a command file to build the mail system.  A
pre-built mail system is also included, having the mail file
as SY:MAIL.XXX.
 
Restrictions: Operating System RT-11 V5.4 or Operating System TSX V6.2
is required because
system calls are required.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
