110707     CONEFR.BAS: Cone Frustrum Layout  Version: February 1984
 
Submitted by: Fred Fortman, National Metal Fabricators, Elk Grove
Village, IL
 
Operating System: RT-11 V2, V3  Source Language: BASIC-11  Memory
Required: 16K minimum  Keywords: Scientific Applications
 
Abstract: The program "CONEFR" (Cone Frustrum) is for
obtaining all the data needed to layout any size cone
frustrum which has a common centerline through the large
and small diameters. The data the program requires is
self explanatory. It will ask for the material
thickness, diameters, vertical height, slant height, or
the angle off the vertical centerline of the side. Any
three of these are all the program requires.
 
There are then options as to the number of segments you
wish to make or the size material you wish to use. Using
the size option the program will give you the number of
segments needed.
 
The data will be shown on the CRT and, if required, will
produce a hard copy of the data on the line printer.
 
Media (Service Charge Code): Two RX01 Diskettes (KB)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
