110104     HDC2: A Finite Element Computer Program for Two-Dimensional
Steady-State Conduction Heat Transfer Analysis  Version: October 1973
 
Submitted by: Howard D. Curtis, Embry-Riddle Aeronautical University,
Daytona Beach, FL
 
Operating System: DOS/BATCH V8.02  Source Language: FORTRAN IV  Memory
Required: 12K minimum  Keywords: Scientific Applications
 
Abstract: The finite element method of two-dimensional
steady-state conduction heat transfer analysis using the
linear-temperature triangular element.
 
Restrictions: Attempts to run in less than 12K, without modification,
will not be successful.
 
Media (Service Charge Code): Write-Up and Listing (DB), 600' Magnetic
Tape (MA)  Format: DOS-11
 
 
