110852     CHPLOT Graphics Printer Package  Version: V1, August 1986
 
Submitted by: Messrs. Tan & Rogers, Medical Physics Dept, Christchurch
Hosp., Christchurch, New Zealand
 
Operating System: RSX-11M V4.0  Source Language: FORTRAN IV, MACRO-11
Memory Required: 64KB  Hardware Required: LA100 or other dot matrix
printer with 'bit addressable' graphics capability.  Keywords:
Graphics, Plotting
 
Abstract: The CHPLOT routines emulate and replace similar routines
written for the old LV-11 electrostatic printer-plotter.
Points, lines, horizontal and vertical characters can be
drawn, and triangular areas can be shaded in any of sixteen
'grey-scale' intensities.  The present package runs on any
of the popular dot-matrix printers, i.e LA100, OKI2410 and
ML84, and C.ITOH1550, and in addition may easily be
modified to run on other printers with
"all-bits-addressable' capability.
 
Media (Service Charge Code): User's Manual (EA), One RX02 Diskette
(LA)  Format: FILES-11, 600' Magnetic Tape (MA)  Format: FILES-11
 
 
