110701     PRINIT: Printer Initialization Routine for the LA120
Printer  Version: V01.0, February 1984
 
Submitted by: Kirk R. Stauffer, Copperweld Robotics, Madison Heights,
MI
 
Operating System: RT-11 V5.0  Source Language: MACRO-11  Memory
Required: 1.5 KW  Hardware Required: LA120 Printer  Keywords:
Utilities - RT-11
 
Abstract: This program remotely configures a Digital Equipment
Corporation LA120 printer from a system terminal. Upon
entry, the printer is initialized with default values
for the horizontal and vertical pitch, form length and
margins. The operator is then able to modify any of
these four parameters from the terminal.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
