110759     PSYCHROM: A Calculating Psychrometric Properties Program
Version: V2.0, August 1984
 
Author: Luther Wilhelm and Robert Freeland, University of Tennessee,
Knoxville, TN
 
Submitted by: Luther Wilhelm
 
Operating System: RT-11  Source Language: FORTRAN IV  Memory Required:
8KW  Keywords: Scientific Applications
 
Abstract: PSYCHROM is a package of subroutines for use in
calculating psychrometric properties. All values are in
SI units. Input combinations of temperature and relative
humidity, temperature and dew point, or temperature and
wet-bulb temperature may be used with appropriate
subroutines to calculate other properties. Properties
calculated (including the two used for calculations)
are: temperature, wet-bulb temperature, dew-point
temperature, relative humidity, enthalpy, specific
volume, humidity ratio, degree of saturation, and
partial pressure of the water vapor. Computational
procedures are based upon recommendations in the ASHRAE
Handbook of Fundamentals (1972). A "test" program
with data is included to verify and compare routines
used for the three possible input combinations.
 
Media (Service Charge Code): Write-Up and Listing (DA), One RX01
Diskette (KA)  Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
