110792     Amway Corporation System Management Tools  Version: March
1985
 
Submitted by: Kreigh Tomaszewski, Amway Corporation, Ada, MI
 
Operating System: RSX-11M-PLUS V1 through V2.1  Source Language:
MACRO-11  Memory Required: 20KW  Software Required: ZZZ will
synchronize with the SRF monitor (GEJAC Inc.) if it is installed, but
SRF is not required.  Hardware Required: PSU requires LA-120
printer(s) defined to the RSX que system as printer despooler(s).
Keywords: System Management - RSX-11
 
Abstract: This program contains a number of system management
utilities
developed and in use on Amway's PDP-11/70 running
RSX-11M-PLUS.
 
ZZZ 	 	A system monitor that will logoff inactive terminals,
		report on pool and activity via a periodic benchmark, limit
		user activity to x% of the cpu, and several other
		functions.  These functions are selected (or not) during a
		generation procedure similar to installing a layered product.
PSU 		A printer utility used to set print characteristics on
		a spooled LA-120.
SCM 		A security CLI that inspects commands prior to passing
		them on to MCR (if the user is authorized for that
		command).  Authorization is done through the IDENT
		field in the RSX account file to allow for on-line changes.
CATCHALL.CMD 	A replacement catchall command file for use
		with the TDX that adds a site library to the supported SYSUIC
		and LIBUIC accounts supported by RSX.
 
Notes: ZZZ links module BLKSUB from MCR.OLB.
 
Restrictions: This software has evolved across all versions of
RSX-11M-PLUS, however, it has not been tested (in its current
version) with releases prior to 2.1.  Since the code has been
conditionalized (by version) it should work on the older
versions of M-PLUS.
 
Complete sources not included.
 
Media (Service Charge Code): Two RX01 Diskettes (KB)  Format:
FILES-11, 600' Magnetic Tape (MA)  Format: FILES-11
 
 
