110294     BASIC-11 Extension Routines  Version: January 1981
 
Submitted by: N. A. Bourgeois, Jr., Sandia National Laboratories,
Albuquerque, NM
 
Operating System: RT-11 V03 or later  Source Language: MACRO-11
Memory Required: 16KW  Software Required: BASIC-11 V2 for RT-11
Keywords: BASIC, Language Interpreters, Programming Languages,
Utilities - RT-11
 
Abstract: This package consists of some extension routines to the
BASIC-11 V2 interpreter running under RT-11 V03 (or
later) that provide the means for reading (GET, GETB,
TBIT) and writing (PUT, PUTB, SBIT) words, bytes and
bits at any implemented UNIBUS or Q-BUS address. This
bus access is useful for exercising any peripheral
device, especially if a handler is not present in the
operating system. The arguments for these routines may
be either octal or decimal. Also included are routines
for identifying (IDEN) the extended BASIC-11 interpreter
and for fast zeroing (NULL) arrays. The package includes
complete source and documentation files.
 
Restrictions: Not usable with double precision option.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
