110851     Extended Character Set  Version: V1, July 1986
 
Submitted by: Dave Garland, Whittier College, Whittier, CA
 
Operating System: RSTS/E  Source Language: BASIC-PLUS  Memory
Required: 16K  Keywords: Plotting
 
Abstract: This program is designed to allow printing (in plot mode) of
both standard and alternate characters.  It is designed for
a CENTRONIX printer but can be used on any other printer
with the same plot mode codes.
 
You may define your own characters or you may use the
characters which have already been defined.  Each file
allows for up to 248 characters.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: DOS-11
 
 
