110810     New Use for Virtual Memory Handler  Version: V1.0, June
1985
 
Submitted by: Tillman B. Smith, United Technologies Research Center,
W. Palm Beach, FL
 
Operating System: RT-11 V5.01B  Source Language: FORTRAN IV  Memory
Required: 512KB  Keywords: Interface Routines
 
Abstract: In real time applications that are I/O bound between local
computers, the VM handler can be used in a different manner
to increase the I/O speed between computers.  The VM handler
organizes the virtual memory into files, and the use of
dual-ported virtual memory provides the local computers with
fast data transfer capability.  Each computer is assigned
its' own write-only and read-only files for I/O data file
exchange.  The file then becomes the basic data packet in the
local information exchange between computer systems.
 
Documentation not available.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
