110865     LOGDIR  Version: V1.1, January 1987
 
Submitted by: Andreas G. Schindler, Darmstadt, Fed. Rep. Germany  D -
6100
 
Operating System: RT-11 V5.1 - 5.3, TSX+, SHARE  Source Language:
FORTRAN IV, MACRO-11  Memory Required: 8/11KW (overlaid/non-overlayed)
Software Required: RT-11 Syslib  Hardware Required: Extended
Instruction Set (EIS)  Keywords: Utilities - Disk - RT-11
 
Abstract: LOGDIR is a special directory program designed to give
directory listings of nested logical disks without mounting
them.  It provides an ANSI mode for use with VT100 like
terminals, producing a "tree of files" in full screen
depiction (similar to the VAX/VMS "Dirtree" utility).  All
directory structured devices that can be accessed via a
RT-11 handler are supported (i.e. disks, VM:'s and LD:'s).
LOGDIR accepts wildcards and a fine choice of switches for
easy file scanning.  Hardcopy output on any device is
supported as well.  The program needs about 11KW of memory
and has been successfully run under RT-11/SJ/FB/XM, TSX+ and
SHARE+.
 
Notes: XM-version provided requiring only l.5KW of low memory.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
