

                                NOTE
                                ----
        TSX-Plus is supported by bootstrapping RT11SJ, RT11FB
        or RT11XM, running RTIME to set the date and time, and
        then booting the mapped system.


The Model 120 Calendar Clock Source Kit contains:

 1) files to build the programs STIME and RTIME, which set the calendar clock
    and initialize your operating system's date and time, respectively,

        RTIME  . COM    RT11/TSX-Plus command file
        STIME  . MAC    Source for STIME for all RT11/TSX-Plus systems
        RTIME  . MAC    Source for RTIME for RT11 V4.0 and later (and TSX-Plus)

 2) subroutines used by RTIME and STIME to read and set the calendar clock,

        CCSUBS . MAC    Source for subroutines used by RTIME


BUILDING RTIME
--------------
To build "STIME", the program which sets the Model 120's time, and "RTIME", the
program which initializes your operating system's clock, invoke the command
file with

 @RTIME

RTIME.COM will create STIME.SAV and RTIME.SAV.

Note that RT does not permit dates prior to 1972.


To set the Model 120 use the "DATE" and/or "TIME" command, then "RUN STIME".


                                  NOTE
                                  ----
 o MACRO.SAV, LINK.SAV, SYSLIB.OBJ and SYSMAC.SML must be present on "SY:".
