         *************************************************************

                           DECUS Symposium RT-11 SIG Tape

                                    Spring, 1984
                                   Cincinnati, OH

                                 Annotated Directory

         *************************************************************

                                      IMPORTANT

                          Read the file, README.1ST, first.

         README.1ST    11  15-Jul-84  SIG tape copy instructions
                                      and new information.

         *************************************************************

         David Stagg
         Dept of Pharmacology
         Yale University Medical School
         333 Cedar Street
         New Haven, CT 06510
         (203) 436-2151

                This is a subdevice handler (necessary for RT-11 Version
         4), used to read the .DSK files on this tape.  See README.1ST for
         an explanation and instructions.

         XD    .SYS     2  05-May-81  SJ/FB driver for V4
         XDATCH.SAV    21  17-Apr-81  XDATCH utility
         DUP   .SXD    41  21-Sep-81  DUP V4.0K patched for XD
         XD    .DOC    10  16-Nov-81  Description document
         XDX   .SYS     2  05-Apr-81  XM driver for V4
         DUP   .COM     1  16-Mar-82  Patch file for V4 DUP.SAV

         XD    .DEV    55  06-Apr-83  VIRTUAL DEVICE for rebuilding XD,
                                        if necessary.
         ************************************************************

         VIRTUL - Subdevice retriever for RSTS.

         E.F.Beadel, Jr., Manager
         CAUSE Instructional Computer Center
         SUNY at Oswego
         Oswego, NY 13126
         (315) 341-3055

                This program allows RSTS/E users to break down the subdev-
         ice files from this tape after they have been copied to disk.  See
         README.1ST for details.

         VIRTUL.BAS 1 File, 28 Blocks
         ************************************************************

                   SPRING 1984 RT SIG TAPE DIRECTORY                 Page 2

         DIR2 - Annotated tape directories, part 2.

         N. A. Bourgeois, Jr.           R. W. Barnard
         Sandia National Laboratories   Sandia National Laboratories
         Division 5238                  Division 7523
         P. O. Box 5800                 P. O. Box 5800
         Albuquerque, NM 87185          Albuquerque, NM 87185
         (505) 844-8088                 (505) 844-5115

                Annotated directories of the DECUS Symposia RT-11 tapes 
         from the Fall of 1981 through the Spring of 1984 (this symposium).
         Previous tapes have DIR1.DSK, which contains annotated directories
         from Spring 1978 through Spring 1981.

         DIR2.DSK 6 Files, 241 Blocks
         ************************************************************

         BENCH* - FORTRAN-77 Benchmark Programs

         Adam Bridge
         Multiware, Inc.
         139 G Street, Suite 161
         Davis CA 95616
         (916) 756-3281

                These are a series of benchmark programs for RT-11 using
         the new FORTRAN-77 compiler. There are versions linked using F77,
         F4 with EIS, F4 with FPU, and F4 with no hardware support.  The
         developers of RT FORTRAN-77 would be interested in knowing the
         results of benchmark tests on as many machines as possible.  If
         you would like to comment, please contact the person listed above.

         BENCH1.DSK 14 Files, 83 Blocks
         BENCH2.DSK 13 Files, 441 Blocks
         BENCH3.DSK 14 Files, 432 Blocks
         BENCH4.DSK 14 Files, 403 Blocks
         BENCH5.DSK 13 Files, 425 Blocks
         ************************************************************

         BUPRES - Read Individual Files from a BUP Magtape

         Michael L. Johnson
         Susan G. Frasier
         Dept. of Pharmacology
         University of Virginia
         Charlottesville, VA 22908
         (804) 924-2496

                BUPRES is a FORTRAN IV program which reads individual files
         from a magnetic tape (MT:) created by the RT-11 version 5
         BACKUP/DEVICE command.  The program supports only single volume
         tapes.  The .SAV file is built for TSX-plus Version 4.1, and FOR-
         TRAN IV version 2.5, but can be rebuilt for other systems, if
         desired.

         BUPRES.DSK 10 Files, 206 Blocks
         ************************************************************

                   SPRING 1984 RT SIG TAPE DIRECTORY                 Page 3

         DSKLB* - Librarian for multiple disks.

         Joel Berez
         Infocom
         64 Jacqueline Rd.
         Waltham, MA 02154
         (617) 492-1031

                Disk Librarian (DSKLIB) is a program to maintain a master
         catalog of multiple disk directories.  Disks are given unique num-
         bers and names, and then placed in the master catalog. A powerful
         Find command is then used to locate a particular file. Full wild-
         cards and multiple switches are supported.  The Archive Handler is
         included here for those persons using RT-11 Version 4 who need
         such a feature.  It has capabilities which complement DSKLIB.  The
         source to DSKLIB is included in this submission.

         DSKLB1.DSK 6 Files, 475 Blocks
         DSKLB2.DSK 11 Files, 40 Blocks
         ************************************************************

         HGRAF* - Plotting Package for RT-11.

         Dennis V. Jensen
         Ames Laboratory ISU/USDOE
         310 Metallurgy
         Ames, IA 50011
         (515) 294-4823

                This is the second DECUS release of HGraph.  It was coded
         entirely in DEC Fortran-66 compatible code.  Included here is a
         new WRTSTR (extracted as WRTST2.*) which will generate characters
         as vectors; it is not dependent on the Visual 550 character gen-
         erator.  Also, there is a cubic spline interpolation line drawing
         routine (extracted as SMOOTH.*) which is compatible with the
         DASHLN calling convention.  Release two is coded in FLECS.  An RT-
         11 FLECS translator is also included for reference.  PLOT3D.FOR is
         included as a separate file.

         HGRAF1.DSK 4 Files, 267 Blocks
         HGRAF2.DSK 3 Files, 356 Blocks
         HGRAF3.DSK 9 Files, 180 Blocks
         ************************************************************

         IMAGE* - RT-11 Natural Image Display Program

         David Fingerhut
         Digital Equipment Corporation
         146 Main Street
         Maynard, MA 01754
         (617) 223-3342

                This program allows the display of photographic (or other
         natural) images on the PRO PC350 computer under RT-11.  Included
         in the submission are the source code to access the PRO graphics
         display, as well as several files of images.

                   SPRING 1984 RT SIG TAPE DIRECTORY                 Page 4

         IMAGE1.DSK 6 Files, 221 Blocks
         IMAGE3.DSK 2 Files, 360 Blocks
         IMAGE4.DSK 2 Files, 360 Blocks
         IMAGE5.DSK 2 Files, 360 Blocks
         IMAGE6.DSK 2 Files, 360 Blocks
         IMAGE7.DSK 2 Files, 360 Blocks
         IMAGE8.DSK 2 Files, 360 Blocks
         IMAGE9.DSK 2 Files, 360 Blocks
         IMAGEA.DSK 2 Files, 360 Blocks
         IMAGEB.DSK 2 Files, 360 Blocks
         ************************************************************

         LA100G - Vector-to-Raster Translator for LA100 Graphics

         Robert Hamilton
         Multiware, Inc.
         139 G St., Suite 161
         Davis, CA 95616
         (916) 756-3291

                LA100G is a program that can read a file of formatted gen-
         eric graphics instructions, translate the instructions into a
         disk-based "bitmap" file, and then create a hardcopy image on one
         of Digital's Letterprinter or Letterwriter 100 serial printers. 
         The program features a dot resolution of up to 1024 by 1024, sim-
         ulated hardware character generation, dotted and dashed line
         generation, and a flexible means for scaling and rotating an
         image.  The input file format is easily user-generated by "post-
         processing" device or metafile output from most any popular
         graphics package.  It can be read with standard FORTRAN READ and
         FORMAT statements.

         LA100G.DSK 13 Files, 282 Blocks
         ************************************************************

         MODEM - Files for Control of DZ(V)11 I/O Lines

         Thomas J. Shinal
         General Scientific Corp.
         1681 East Gude Dr.
         Rockville, MD 20850
         (301) 340-2773

                These files allow a DIBOL user to control the characteris-
         tics of the DZ11 and DZV11 serial interface boards.  These include
         modem-controlling functions, such as DTR, etc.  The routines are
         written in MACRO and DIBOL.

         MODEM.DSK 7 Files, 25 Blocks
         ************************************************************

         RESEQ - FORTRAN Program Line Number Resequencer

         R. W. Barnard
         Sandia National Laboratories
         Division 7523
         Albuquerque, NM 87185
         (505) 844-5115

                   SPRING 1984 RT SIG TAPE DIRECTORY                 Page 5

                This program is an enhancement and modification of one ori-
         ginally submitted to the RT-11 SIG tape in 1980 by Larry Morton. 
         It will renumber the statements of FORTRAN-IV and FORTRAN-77 pro-
         grams to give them a nice order.  The starting statement number
         and increment are specifiable.

                Also included are some SYSLIB routines for easier conver-
         sion to FORTRAN-77.  SYSLIB has the string-handling routines INDEX
         and LEN, for byte variables.  FORTRAN-77 has two intrinsic routi-
         nes of the same names for character variables.  To aid in the
         conversion of FORTRAN-IV routines to F-77, two routines (INDEXB
         and LENB), can be added to SYSLIB which have the same functional-
         ity as the SYSLIB routines INDEX and LEN, so all references in
         FORTRAN-IV programs can be changed to these new calls.

         RESEQ.DSK 13 Files, 170 Blocks
         ************************************************************

         RUNOF* - Bonner Lab RUNOFF, Version 5.1

         John M. Clement
         Bonner Lab, Rice University
         P. O. Box 1892
         Houston, TX 77401
         (713) 527-4018

                Bonner Lab Runoff is a text formatter which when used with
         your favorite editor makes a complete word processor.  Its syntax
         is almost a complete emulation of DSR (Digital Standard Runoff)
         and it is very compatible with previous versions of Runoff.  The
         intent of this program is to support complete scientific word
         processing to produce publication quality output.

                This version allows complete control of any special printer
         available via user definable escape sequences.  In addition a
         macro facility allows text or sequences of commands to be abbrevi-
         ated to a single label.  If the printer has the correct features
         then variable spacing, subscripting, superscripting, and equation
         formatting are possible.  By properly defining escape sequences
         the user may support different printers in a transparent fashion.

                Table of contents, indexing and sub-indexing are all sup-
         ported.  Multiple table of contents or multiple indexing may be
         constructed from the available commands.  A variety of LAYOUT and
         STYLE commands may completely change the look of the pages.  Table
         layout is simplified by right justified and 'decimal' justified
         tabs.  Permanent margins which apply to the page headers are
         available.  These simplify the setting of header and  text mar-
         gins.  This runs under VMS, RSX, IAS, RT11, TSX, and probably
         RSTS.

         RUNOF1.DSK 108 Files, 480 Blocks
         RUNOF2.DSK 21 Files, 482 Blocks
         RUNOF3.DSK 63 Files, 476 Blocks
         RUNOF4.DSK 5 Files, 136 Blocks
         ************************************************************

                   SPRING 1984 RT SIG TAPE DIRECTORY                 Page 6

         TSXLIB - Programmed Requests for TSX+

         N. A. Bourgeois, Jr.
         NAB Software Services, Inc.
         P. O. Box 20009
         Albuquerque, NM 87154
         (505) 298-2346

                This is an update of the TSX+ system services available via
         programmed requests.  They are in the form of a library, available
         to the FORTRAN programmer.  The library has been updated to in-
         clude all EMT's through TSX+ Version 5.0.

         TSXLIB.DSK 18 Files, 490 Blocks
         ************************************************************

         UCLPLS - User Command Language (UCL) Program.

         William K. Walker
         Monsanto Research Corp.
         P. O. Box 32    OS-123
         Maimisburg, OH  45342
         (513) 865-3557

                UCL+ is upward-compatible with the UCL distributed with
         RT-11, Version 5.01B.  It contains a number of extensions, includ-
         ing chaining to additional UCL's, "run-by-name", path definition,
         display of command expansions, etc.  Symbols are defined by enter-
         ing a "symbol definition string" in the format:
         symbol==definition.

         UCLPLS.DSK 11 Files, 293 Blocks
         ************************************************************

         UCLTSX - User Command Language (UCL) Program.

         William Davidson
         Sandia National Laboratories
         Albuquerque, NM 87185

                This is an implementation of a UCL which allows RT-11 com-
         mand files to be treated in the same fashion as TSX+ command
         files.  With this UCL, unrecognized keyboard entries are processed
         in the same order under RT as they would be under TSX+.

         UCLTSX.DSK 15 Files, 100 Blocks
         ************************************************************

         UNMAC - Object File to Source File Translator

         Robert Walraven
         University of California
         Applied Science
         Davis, CA 95616
         (916) 752-3300

                UNMAC is a FORTRAN program to convert an RT-11 object file
         into a source or listing file.  Object files are much more useful

                   SPRING 1984 RT SIG TAPE DIRECTORY                 Page 7

         to decode then SAV files because they contain information such as
         subroutine names, variable names, psect info, etc.  This distribu-
         tion contains complete sources and a command file for building
         UNMAC.  The file UNMAC7.SAV is an executable version that was
         built with the FORTRAN-77 compiler.

         UNMAC.DSK 14 Files, 297 Blocks
         ************************************************************

         BIBLE*, BOOK** - The King James Version of the Bible

         Submitted by:
         Dean Lampman
         STARFLO, Inc,
         #5 Hickory Wood Drive
         Cincinnati, OH 45140
         (513) 683-4871

                The files labeled BIBLE*.DSK are subdevices containing sev-
         eral books of the Bible.  The files labeled BOOK**.LST are
         individual books.  This was converted to magnetic media by an opt-
         ical scanner.  Users are cautioned that there may have been
         conversion errors.

         BOOK01.LST 409 Blocks
         BOOK02.LST 351 Blocks
         BOOK03.LST 262 Blocks
         BOOK04.LST 365 Blocks
         BOOK05.LST 303 Blocks
         BIBLEA.DSK 3 Files, 438 Blocks
         BOOK09.LST 267 Blocks
         BIBLEB.DSK 2 Files, 482 Blocks
         BIBLEC.DSK 2 Files, 481 Blocks
         BIBLED.DSK 2 Files, 371 Blocks
         BIBLEE.DSK 3 Files, 381 Blocks
         BOOK19.LST 475 Blocks
         BIBLEF.DSK 3 Files, 259 Blocks
         BOOK23.LST 402 Blocks
         BOOK24.LST 461 Blocks
         BIBLEG.DSK 2 Files, 462 Blocks
         BIBLEH.DSK 13 Files, 460 Blocks
         BIBLEI.DSK 2 Files, 426 Blocks
         BIBLEJ.DSK 2 Files, 486 Blocks
         BIBLEK.DSK 3 Files, 478 Blocks
         BIBLEL.DSK 19 Files, 476 Blocks
         BOOK66.LST 129 Blocks
         ************************************************************

         The Spring, 1984, RT SIG tape contains 66 Files, 19824 Blocks.
         It was prepared by:                    It is distributed by:

         R. W. Barnard                          Thomas J. Shinal
         Sandia National Laboratories           General Scientific Corp.
         Division 7523                          1681 East Gude Dr.
         P. O. Box 5800                         Rockville MD 20850
         Albuquerque, NM 87185                  (301) 340-2773
         15-July-1894

