CC     JOB   TEST CARRIAGE CONTROLS
       ORG   500
START  CS    332
       CS    
       MLCWA @TEST OF CARRIAGE CONTROLS@,250
       W     
       CS    299
       H
       MLCWA @IMMEDIATE SPACE TESTS@,250
       W
       CS    299
* SINGLE SPACE
       MLCWA XXX,270
       W
       W
       CS    299
       MLCWA @ABOVE SHOULD BE ON ADJACENT LINES@,270
       W
       CS    299
* DOUBLE SPACE
       MLCWA XXX,270
       W
       CC    J                               SINGLE SPACE IMMEDIATE
       W
       CS    299
       MLCWA @ABOVE SHOULD BE SEPARATED BY ONE LINE@,270
       W
       CS    299
* TRIPLE SPACE
       MLCWA XXX,270
       W
       CC    K                               DOUBLE SPACE IMMEDIATE
       W
       CS    299
       MLCWA @ABOVE SHOULD BE SEPARATED BY TWO LINES@,270
       W
       CS    299
* QUADRUPLE SPACE
       MLCWA XXX,270
       W
       CC    L                               TRIPLE SPACE IMMEDIATE
       W
       CS    299
       MLCWA @ABOVE SHOULD BE SEPARATED BY THREE LINES@,270
       W
       CS    299
*
       MLCWA @DEFERRED SPACE TESTS@,250
       W
       CS    299
* SINGLE SPACE
       MLCWA XXX,270
       W
       W
       CS    299
       MLCWA @ABOVE SHOULD BE ON ADJACENT LINES@,270
       W
       CS    299
* DOUBLE SPACE
       MLCWA XXX,270
       CC    /                               SINGLE SPACE DEFERRED
       W
       W
       CS    299
       MLCWA @ABOVE SHOULD BE SEPARATED BY ONE LINE@,270
       W
       CS    299
* TRIPLE SPACE
       MLCWA XXX,270
       CC    S                               DOUBLE SPACE DEFERRED
       W
       W
       CS    299
       MLCWA @ABOVE SHOULD BE SEPARATED BY TWO LINES@,270
       W
       CS    299
* QUADRUPLE SPACE
       MLCWA XXX,270
       CC    T                               TRIPLE SPACE DEFERRED
       W
       W
       CS    299
       MLCWA @ABOVE SHOULD BE SEPARATED BY THREE LINES@,270
       W
       CS    299
*
       MLCWA @END OF CARRIAGE TESTS@,250
       W
       CS    299
       H     *-3
*
XXX    DCW   @XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX@
       END   START


