	.TITLE SYSBLK
 
/ .... EDIT #2 .... 23 FEB 70
 
/ COPYRIGHT 1969, 1970 DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASS.
 
/ PDP-9 BACKGROUND FOREGROUND SYSTEM.
 
/ SPECIAL SYSTEM PROGRAM BLOCK (BLOCK 101) WITH 4-WORD ENTRY PER PROGRAM.
 
/ ORDERING OF PROGRAMS MUST NOT CHANGE. LOGICAL CODES FOR PROGRAM
/	NAMES, CORRESPONDING TO LOCATION IN SYSBLK, ARE USED BY
/	BFKM9 (NON-RESIDENT MONITOR), .SYSLD (SYSTEM LOADER),
/	AND PATCH (SYSTEM PATCHER).
 
/	WD0	LOGICAL BLOCK #
/	WD1	LOAD ADDRESS (13 BITS)
/	WD2	PROGRAM SIZE (2'S COMP.)
/	WD3	START ADDRESS (13 BITS)
 
	.ABS
	.LOC 0
 
/LOAD, DDT		/0 (RELOCATABLE)
	0
	0
	0
	0
/EDIT V7A			/1 (13 OCTAL BLKS)
	656
	12577
	772577
	13000
/MACRO BF6A		/2 (27 OCTAL BLKS)
	742
	5000
	765000
	5000
/PIP V9A			/3 (20 OCTAL BLKS)
	671
	10051
	770051
	10051
/F4 V8A			/4 (31 OCTAL BLKS)
	711
	3626
	763626
	4304
/SGEN			/5 (RELOCATABLE)
	0
	0
	0
	0
/DUMP V3A			/6 (4 OCTAL BLKS)
	1044
	16000
	776142
	16000
/UPDATE V6A		/7 (14 OCTAL BLKS)
	1050
	13670
	773670
	13671
/CONV V3A			/10 (14 OCTAL BLKS)
	1064
	12000
	772142
	12000
/MACROA BF5A		/11 (24 OCTAL BLKS)
	1020
	6320
	766320
	6320
/F4A V8A			/12 (27 OCTAL BLKS)
	771
	5150
	765150
	5567
/EXECUTE(E) V2A		/13 (RELOCATABLE)
	0
	0
	0
	0
/CHAIN V2A		/14 (20 OCTAL BLKS)
	630
	10000
	770000
	10000
/PATCH V4A		/15 (6 OCTAL BLKS)
	650
	15236
	775400
	15236
/RESMON			/16 (56 OCTAL BLKS)
	0
	0
	760100
	100
/BFKM9 V1A		/17 (20 OCTAL BLKS)
	102
	12000
	772000
	12000
/.SYSLD V1A		/20 (13 OCTAL BLKS)
	56
	14000
	774000
	14000
 
	.END
