	.TITLE	FLOATJ (DBLEJ) J TO REAL (OR D.P. REAL) CONVERSION
/ 
/ 
/                   FIRST PRINTING, FEBRUARY 1974
/ 
/ THE INFORMATION IN THIS DOCUMENT IS SUBJECT TO 
/ CHANGE WITHOUT NOTICE AND SHOULD NOT BE CONSTRUED
/ AS A COMMITMENT BY DIGITAL EQUIPMENT CORPORATION.
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPON-
/ SIBILITY FOR ANY ERRORS THAT MAY APPEAR IN THIS
/ DOCUMENT.
/ 
/ THE SOFTWARE DESCRIBED IN THIS DOCUMENT IS FUR-
/ NISHED TO THE PURCHASER UNDER A LICENSE FOR USE ON
/ A SINGLE COMPUTER SYSTEM AND CAN BE COPIED (WITH
/ INCLUSION OF DIGITAL'S COPYRIGHT NOTICE) ONLY FOR 
/ USE IN SUCH SYSTEM, EXCEPT AS MAY OTHERWISE BE PRO-
/ VIDED IN WRITING BY DIGITAL.
/ 
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPONSIBILITY
/ FOR THE USE OR RELIABILITY OF ITS SOFTWARE ON EQUIP-
/ MENT THAT IS NOT SUPPLIED BY DIGITAL.
/ 
/ COPYRIGHT (C) 1974, BY DIGITAL EQUIPMENT CORPORATION
/ 
/ 
        .EJECT
/COPYRIGHT 1971, DIGITAL EQUIPMENT CORP., MAYNARD, MASS.
/FOR HARDWARE FLOATING POINT PROCESSOR (FPP), DEFINE 90 FPP,
/EDIT #001  6-17-71
	.GLOBL	FLOATJ, DBLEJ, .DA,
	.IFUND %FPP
	.GLOBL .JG, .JW
	.ENDC
	.IFDEF %FPP
ELF=714110
	.ENDC
/CALLING SEQUENCE--
/	JMS*	FLOATJ (DBLEJ)
/	JMP	.+2
/	.DSA	ARG ADDR.	/BIT #0=1 IF INDIRECT
DBLEJ=.
FLOATJ	0
	JMS*	.DA
	JMP	FLTJ02
FLTJ01	0
FLTJ02=.
	.IFDEF %FPP
	ELF
	.DSA FLTJ01+400000
	.ENDC
	.IFUND %FPP
	JMS*	.JG		/LD. J INTO AC,MQ
	.DSA	FLTJ01+400000	/ARG.
	JMS*	.JW		/AC,MQ TO FPAC
	.ENDC
	JMP*	FLOATJ
	.END
