	.TITLE ADCON - AD15 CONNECT.
/ 
/ 
/                   FIRST PRINTING, FEBRUARY 1974
/ 
/ THE INFORMATION IN THIS DOCUMENT IS SUBJECT TO 
/ CHANGE WITHOUT NOTICE AND SHOULD NOT BE CONSTRUED
/ AS A COMMITMENT BY DIGITAL EQUIPMENT CORPORATION.
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPON-
/ SIBILITY FOR ANY ERRORS THAT MAY APPEAR IN THIS
/ DOCUMENT.
/ 
/ THE SOFTWARE DESCRIBED IN THIS DOCUMENT IS FUR-
/ NISHED TO THE PURCHASER UNDER A LICENSE FOR USE ON
/ A SINGLE COMPUTER SYSTEM AND CAN BE COPIED (WITH
/ INCLUSION OF DIGITAL'S COPYRIGHT NOTICE) ONLY FOR 
/ USE IN SUCH SYSTEM, EXCEPT AS MAY OTHERWISE BE PRO-
/ VIDED IN WRITING BY DIGITAL.
/ 
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPONSIBILITY
/ FOR THE USE OR RELIABILITY OF ITS SOFTWARE ON EQUIP-
/ MENT THAT IS NOT SUPPLIED BY DIGITAL.
/ 
/ COPYRIGHT (C) 1974, BY DIGITAL EQUIPMENT CORPORATION
/ 
/ 
        .EJECT
/COPYRIGHT 1971, DIGITAL EQUIPMENT CORP.,MAYNARD MASS.
/W.A. DESIMONE.
/
/EDIT 001 11-12-71
/
/
/CALLING SEQUENCE:	CALL ADCON(LUN,IEV)
/
/	JMS*	ADCON
/	JMP .+3		/SUBR. RETURN.
/	ADRR. OF LUN.
/	ADDR. OF EV	/OPTIONAL
/	NEXT INSTR.
/
/ADCON(LUN,IEV) - QUEUE ADCON I/O REQUEST TO CONNECT AD15 HANDLER
/TASK TO REQUESTING TASK.  THIS CALL MUST BE MADE BEFORE ANY OTHER QUEUE I/O REQUESTS
/TO AD15 HANDLER TASK ARE MADE (EXCEPT HINF).  
/
	.EJECT
/
	.GLOBL ADCON,.DA
/
ADCON	0		/SUBR. ENTRY.
	JMS*	.DA
	JMP	ARGEND
LUN	0		/ADDR. OF LUN.
EV	0		/ADDR. OF EV.
ARGEND	LAC*	LUN
	DAC	CPB2
	LAC	EV
	DAC	CPB1
	DZM	EV	/REINIT.
	CAL	CON
	JMP*	ADCON	/EXIT
/
/ADCON CPB.
/
CON	500	/FUNCT. CODE.
CPB1	0	/EV.
CPB2	0	/LUN.
	.END
