
                       Fog Library Disk FOG-DOS.355
Copyright (1990) by Fog International Computer Users Group to the extent 
not copyrighted by the original author for the exclusive use and enjoyment 
of its members. Any reproduction or distribution for profit or personal 
gain is strictly forbidden. 

For information, contact FOG, P. O. Box 3474, Daly City, CA. 94015-0474.

<SHAREWARE> as part of the description of a file indicates that the program 
is distributed on a "try first, pay if you like it" basis. If you find the 
program(s) meet your need, please refer to the author's documentation for 
information on becoming a registered user. Only by registering and paying 
for the programs you like and use will the authors of such programs continue 
development. Often, more complete documentation, additional modules, and new 
releases are available only to registered users.


Advanced disk utilities. Use these programs with care!

Filename     Description
-01-10  .90  This is the release date of the disk.
-DOS355 .DOC This is the description of the disk contents.
FAT     .EXE  15191 ver. 1.05    [FAT Display 1 of 2]
             Displays the chain of clusters (disk allocation units) that
             belong to a disk file to determine which file "owns" a
             specific cluster or sector. Also displays general information
             about a disk. Does not perform any functions that alter the
             disk data; it is an inquiry program only.
FAT     .DOC   7759 ver. 1.05    [FAT Display 2 of 2]
FAT_PRNT.BAS   4480 ver. 8/15/82 [FAT Print 1 of 2]
             Basic program which prints the file allocation table and
             directory information from a disk. Requires that the "S"
             flag be set to 512.
FAT_PRNT.DOC    212 ver. 8/15/82 [FAT Print 2 of 2]
GULP    .EXE  17920 ver. 8/13/87 [Guld 1 of 2]
             File device filling utility which writes one file filling the
             entire disk and then erases that file. This will make it
             impossible to UNERASE deleted files on the disk and removes
             all traces of your files from the disk.
GULP    .DOC   1024 ver. 8/13/87 [Guld 2 of 2]
PACKDISK.COM   4549 ver. 1.2     [PackDisk Utilities 1 of 7] <SHAREWARE>
             Eliminates file fragmentation on the drive, unallocated space
             between files and then re-integrates lost clusters (file
             allocation units into the available space on the disk. Also
             packs the root directory and subdirectories and frees
             trailing clusters.
DELDIR  .COM   3110 ver. 1.2     [PackDisk Utilities 2 of 7] <SHAREWARE>
             Deletes a subdirectory together with its files and sub-
             directories.
LISTFRAG.COM   2798 ver. 1.2     [PackDisk Utilities 3 of 7] <SHAREWARE>
             Lists all fragmented files on the drive.
NAMEDIR .COM   2909 ver. 1.2     [PackDisk Utilities 4 of 7] <SHAREWARE>
             Renames a subdirectory.
TRANSDIR.COM   3821 ver. 1.2     [PackDisk Utilities 5 of 7] <SHAREWARE>
             Transfers a subdirectory together with its files and
             subdirectory into another directory on the same drive.
PARK    .COM    372 ver. 1.2     [PackDisk Utilities 6 of 7] <SHAREWARE>
             Parks disk(s) before power off.
PACKDISK.DOC  23415 ver. 1.2     [PackDisk Utilities 7 of 7] <SHAREWARE>
BOOTSEC .EXE  10274 ver. 5/30/86 [Boot Sector 1 of 3]
             Extracts standard disk information that is placed in the boot
             sector of most disks and prints it to the screen. Includes
             'C' source.
BOOTSEC .C     2982 ver. 5/30/86 [Boot Sector 2 of 3]
BOOTSEC .DOC    446 ver. 5/30/86 [Boot Sector 3 of 3]
BT      .COM   1493 ver. 1.06    [BootThru 1 of 3]
             Modify a floppy disk's boot sector so that the boot process
             will "fall through" to the hard disk. This avoids the need to
             be sure the drive door is open.
BT      .ASM   9756 ver. 1.06    [BootThru 2 of 3]
BT      .DOC   1691 ver. 1.06    [BootThru 3 of 3]
DEFRAG  .BAS   5888 ver. 1.9
             A Basic program to defragment your drive.
DTL     .EXE   6768 ver. 10/1/87 [Drive Table List 1 of 2]
             Formats and displays the contents of your ROM's disk type
             table, showing the number of cylinders, heads and other
             drive characteristics defined for each drive type known to
             SETUP. Does not work on XT systems.
DTL     .DOC    827 ver. 10/1/87 [Drive Table List 2 of 2]
DISKPACK.EXE  23936 ver. 1.02    [Disk Pack 1 of 2]
             Pack fragmented disks by storing contiguous disk clusters
             with no unused cluster gaps between files. All directory
             entries are arranged so that hidden, system or VOLUME-ID
             attributes are placed at the beginning of a directory (in the
             root directory, the are left as is; in all others they are
             arranged alphabetically). Subdirectories in alphabetic order
             are next and then all other directory entries, sorted by name
             follow. Erased entries are discarded.
DISKPACK.DOC  10478 ver. 1.02    [Disk Pack 2 of 2]
DTST    .EXE   7074 ver. 1.0     [Disk Tester 1 of 3]
             Check out your hard disks. This has the special ability to
             report "slow" sectors (ones requiring retries). Turbo 'C'
             source is included.
DTST    .C     3157 ver. 1.0     [Disk Tester 2 of 3]
DTST    .DOC   1112 ver. 1.0     [Disk Tester 3 of 3]
LISTBAD .COM    691 ver. 1.23    [List Bad Clusters 1 of 3] <SHAREWARE>
             Gives a list of all the clusters on a disk that are marked as
             bad. ASM source is included.
LISTBAD .ASM   9768 ver. 1.23    [List Bad Clusters 2 of 3] <SHAREWARE>
LISTBAD .DOC   2321 ver. 1.23    [List Bad Clusters 3 of 3] <SHAREWARE>
VCOPY   .EXE  18832 ver. 1.30    [Verify Copy 1 of 2] <SHAREWARE>
             Replacement for DOS COPY command which compares the CRC value
             of the source file against the CRC of the resulting
             destination file. Also checks to see if the file name is
             already in use on the destination disk. Can also be used to
             move a file from one subdirectory to another.
VCOPY   .DOC  16256 ver. 1.30    [Verify Copy 2 of 2] <SHAREWARE>
WPHD    .COM    437 ver. Oct2185 [Write Protect Disk 1 of 2]
             Use this to write and format protect your hard disk. Useful
             for testing new software without danger that something will
             be written to the drive. This just toggles the INT 13.
WPHD    .DOC   1280 ver. Oct2185 [Write Protect Disk 2 of 2]
FORMAT  .BAT   1024 A batch file to force inclusion of A or B drive
             identifier. Requires that your FORMAT program be renamed to
             4MAT. Useful to protect novices from accidentally formatting
             the hard disk. Modify it if you only want to permit
             formatting on one or the other of the drives.
SPINTEST.COM   3002 ver. 1.2     [Sector Interleave 1 of 2]
             Steve Gibson's Sector Interleave Performance Diagnostic test
             is used to determine the performance of hard disk systems.
             This is part of the SPINRITE package but only this piece may
             be freely exchanged.
SPINTEST.DOC   2192 ver. 1.2     [Sector Interleave 2 of 2]
AUTOPARK.COM    943 ver. 5/3/86  [Autopark Hard Disk 1 of 3]
             Park the hard disks heads when the drive is not in use. Just
             add this to your AUTOEXEC.BAT file and inactivity will get
             your heads parked. Probably not needed on newer drives.
             ASM source is included.
AUTOPARK.ASM  21625 ver. 5/3/86  [Autopark Hard Disk 2 of 3]
AUTOPARK.DOC   2434 ver. 5/3/86  [Autopark Hard Disk 3 of 3]
COMMENT .SYS    332 ver. 5/19/85 [Comment to printer 1 of 3]
             A MS-DOS 2.0+ device driver whose function is simply to echo
             a string to the standard output device. Simply add this to
             your CONFIG.SYS. ASM source is included
COMENT  .ASM  11136 ver. 5/19/85 [Comment to printer 2 of 3]
COMMENT .DOC   2795 ver. 5/19/85 [Comment to printer 3 of 3]
