Previous [TOC] Next

| Opcode Index

    ACD..............Add Cardinal to Double

    ADC..............Add Double to Cardinal

    ADD..............Add

    ADDSB............Add Signed Byte

    AF...............Allocate Frame

    AL0IB............Add Local Zero to Immediate Byte

    AND..............And

    BITBLT...........Bit Block Transfer

    BLECL............Block Equal Code Long

    BLEL.............Block Equal Long

    BLT..............Block Transfer

    BLTC.............Block Transfer Code

    BLTCL............Block Transfer Code Long

    BLTL.............Block Transfer Long

    BLTLR............Block Transfer Long Reversed

    BNDCK............Bounds Check

    BNDCKL...........Bounds Check Long

    BRK..............Break

    BYTBLT...........Byte Block Transfer

    BYTBLTR..........Byte Block Transfer Reversed

    CATCH............Catch

    CKSUM............Checksum

    DADD.............Double Add

    DBL..............Double

    DCMP.............Double Compare

    DDBL.............Double Double

    DDUP.............Double Duplicate

    DEC..............Decrement

    DEXCH............Double Exchange

    DINC.............Double Increment

    DIOR.............Double Inclusive Or

    DIS..............Discard

    DIS2.............Discard Two

    DMUL.............Double Multiply

    DSHIFT...........Double Shift

    DSK..............Dump Stack

    DSUB.............Double Subtract

    DUP..............Duplicate

    DXOR.............Double Exclusive Or

    EFCB.............External Function Call Byte

    EFCn.............External Function Call n

    EXCH.............Exchange

    EXDIS............Exchange Discard

    FF...............Free Frame

    GAB..............Global Address Byte

    GAn..............Global Address n

    GAW..............Global Address Word

    GMF..............Get Map Flags

    INC..............Increment

    IOR..............Inclusive Or

    JB...............Jump Byte

    JDEB.............Jump Double Equal Byte

    JEB..............Jump Equal Byte

    JEBB.............Jump Equal Byte Byte

    JEP..............Jump Equal Pair

    JGB..............Jump Greater Byte

    JGEB.............Jump Greater Equal Byte

    JIB..............Jump Indexed Byte

    JIM..............Jump Indexed Word

    JLB..............Jump Less Byte

    JLEB.............Jump Less Equal Byte

    Jn...............Jump n

    JNEB.............Jump Not Equal Byte

    JNEBB............Jump Not Equal Byte Byte

    JNEP.............Jump Not Equal Pair

    JNZB.............Jump Not Zero Byte

    JNZn.............Jump Not Zero n

    JS...............Jump Stack

    JUGB.............Jump Unsigned Greater Byte

    JUGEB............Jump Unsigned Greater Equal Byte

    JULB.............Jump Unsigned Less Byte

    JULEB............Jump Unsigned Less Equal Byte

    JW...............Jump Word

    JZB..............Jump Zero Byte

    JZn..............Jump Zero n

    KFCB.............Kernel Function Call Byte

    LAB..............Local Address Byte

    LAn..............Local Address n

    LAW..............Local Address Word

    LFC..............Local Function Call

    LGB..............Load Global Byte

    LGDB.............Load Global Double Byte

    LGDn.............Load Global Double n

    LGn..............Load Global n

    LIB..............Load Immediate Byte

    LIHB.............Load Immediate High 8yte

    LINB.............Load Immediate Negative Byte

    LINI.............Load Immediate Negative Infinity

    LINn.............Load Immediate n

    LINT.............Lengthen Integer

    LI00.............Load Immediate Double Zero

    LIW..............Load Immediate Word

    LKB..............Link Byte

    LLB..............Load Local Byte

    LLDB.............Load Local Double Byte

    LLDn.............Load Local Double n

    LLKB.............Load Link Byte

    LLn..............Load Local n

    LIN1.............Load Immediate Negative One

    LP...............Lengthen Pointer

    LSK..............Load Stack

    LUDIV............Long Unsigned Divide

    MUL..............Multiply

    NEG..............Negate

    NILCKL...........Nil Check Long

    PI...............Port In

    PLB..............Put Local Byte

    PLD0.............Put Local Double Zero

    PLDB.............Put Local Double Byte

    PLn..............Put Local n

    PO...............Port Out

    POR..............Port Out Responding

    PS0F.............Put Swapped Zero Field

    PSB..............Put Swapped Byte

    PSDB.............Put Swapped Double Byte

    PSDLB............Put Swapped Double Long Byte

    PSDO.............Put Swapped Double Zero

    PSF..............Put Swapped Field

    PSLB.............Put Swapped Long Byte

    PSLF.............Put Swapped Long Field

    RB...............Read Byte

    RC...............Read Code

    RCFS.............Read Code Field Stack

    RDB..............Read Double Byte

    RDLB.............Read Double Long Byte

    RDLO.............Read Double Long Zero

    RDO..............Read Double Zero

    REC..............Recover

    REC2.............Recover Two

    RET..............Return

    RF...............Read Field

    RGILP............Read Global Indirect Long Pair

    RGIP.............Read Global Indirect Pair

    RKDIB............Read Link Double Indirect Byte

    RKIB.............Read Link Indirect Byte

    RL0F.............Read Long Zero Field

    RLB..............Read Long Byte

    RLDILP...........Read Local Double Indirect Long Pair

    RLDIOO...........Read Local Double Indirect Zero Zero

    RLDIP............Read Local Double Indirect Pair

    RLF..............Read Long Field

    RLFS.............Read Long Field Stack

    RLI0n............Read Local Indirect Zero n

    RLILP............Read Local Indirect Long Pair

    RLILPF...........Read Local Indirect Long Pair Field

    RLIP.............Read Local Indirect Pair

    RLIPF............Read Local Indirect Pair Field

    RLO..............Read Long Zero

    RLS..............Read Long String

    Rn...............Read n

    ROB..............Read Overhead Byte

    ROF..............Read Zero Field

    ROTATE...........Rotate

    RRIT.............Read Register IT

    RRMDS............Read Register MDS

    RRPSB............Read Register PSB

    RRPTC............Read Register PTC

    RRWDC............Read Register WDC

    RRWP.............Read Register WP

    RRXTS............Read Register XTS

    RS...............Read String

    SCB..............Store Global Byte

    SDDIV............Signed Double Divide

    SDIV.............Signed Divide

    SFC..............Stack Function Call

    SGDB.............Store Global Double Byte

    SHIFT............Shift

    SHIFTSB..........Shift Signed Byte

    SLB..............Store Local Byte

    SLDB.............Store Local Double Byte

    SLDn.............Store Local Double n

    SLn..............Store Local n

    SM...............Set Map

    SMF..............Set Map Flags

    SUB..............Subtract

    TRPL.............Triple

    TXTBLT...........Text Block Transfer

    UDCMP............Unsigned Double Compare

    UDDIV............Unsigned Double Divide

    UDIV.............Unsigned Divide

    W0...............Write Zero

    W0F..............Write Zero Field

    WB...............Write Byte

    WDB..............Write Double Byte

    WDLB.............Write Double Long Byte

    WF...............Write Field

    WLB..............Write Long Byte

    WLDILP...........Write Local Double Indirect Long Pair

    WLF..............Write Long Field

    WLFS.............Write Long Field Stack

    WLlLP............Write Local Indirect Long Pair

    WLlP.............Write Local Indirect Pair

    WLOF.............Write Long Zero Field

    WLS..............Write Long String

    WOB..............Write Overhead Byte

    WRIT.............Write Register IT

    WRM..............Write Register MP

    WRMDS............Write Register MDS

    WRPSB............Write Register PSB

    WRPTC............Write Register PTC

    WRWDC............Write Register WDC

    WRWP.............Write Register WP

    WRXTS............Write Register XTS

    WS...............Write String

    WSOF.............Write Swapped Zero Field

    XE...............XFER and Enable

    XF...............XFER and Free

    XOR..............Exclusive Or

Previous [TOC] Next

[last edited 4/11/99 10:03PM]