# Interdata Simulator Configuration

Interdata was founded in the mid 1960's. It produced a family of 16b minicomputers loosely modeled on the IBM 360 architecture. Microprogramming allowed a steady increase in the functionality of successive models.

- Interdata 3
- Interdata 4 (autoload, floating point)
- Interdata 5 (list processing, microcoded automatic I/O channel)
- Interdata 70, 74, 80
- Interdata 6/16, 7/16
- Interdata 8/16, 8/16e (double precision floating point, extended memory)

In the early 1970's, Interdata was purchased by Perkin-Elmer. In 1974, it introduced one of the first 32b minicomputers, the 7/32. Several generations of 32b systems followed:

- Interdata 7/32
- Interdata 8/32
- Perkin-Elmer 3205, 3210, 3220
- Perkin-Elmer 3250

Interdata was spun out of Perkin-Elmer as Concurrent Computer Corporation.

Photographs:

- Interdata 4 (courtesy of Carl Friend)
- Interdata 70 (courtesy of Tony Farrell)
- Interdata 70 front panel detail (courtesy of Tony Farrell)

##

Option | Description | Capacity
16b CPU and memory | Interdata 3, 4, 7/16, 8/16, 8/16e | 8KB-64KB (256KB on 8/16e)
32b CPU and memory | Interdata 7/32, 8/32 | 64KB-1024KB
32b options | double precision floating point |
DMA | Selector channels | 1-4
Console | KSR-33 Teletype |
| PASLA-based terminal |
Paper tape | reader and punch |
Clocks | line time clock |
| precision real-time clock |
Line printer | line printer |
Terminal multiplexor | PASLA-based terminal multiplexor | 32 lines
Disk | floppy disk | 256KB
| cartridge disk | 2.5MB/10MB
| mass storage module controller | 13.5MB - 268MB
Magnetic tape | 9 track magnetic tape |

Updated 18-Jun-2003 by Bob Supnik (bob AT supnik DOT org - anti-spam encoded)