« Установка UNIX v7 И снова про BASIC-PLUS-2 »
FORTRAN-77 5.4
Как то я уже писал про установку FORTRAN-77 в RSX11M+ только версии 5.3 которая не совсем подходит, хотелось версию посвежее да еще и с установленными патчами.
Версия 5.4 все же нашлась и успешно установилась.
Ниже показана установка с устройства RL02 на котором лежит образ ленты F77V54.TAP
>MOU DL0: F77
>VCP CREATE /UNIT=3/ALT
>VCP CON DL0:[F77]F77V54.TAP/TAP/DRV:MU:/RO/MOU:FOR
VCP - Device VF0: (MU1:) has been assigned.
>INS $BRU
>BRU /REW/UFD/NOI/NEW/BAC:aut101.a MU1: DU0:
BRU - Starting Tape 1 on MU1:
BRU - End of Tape 1 on MU1:
BRU - Completed
>SET /UIC=[367,367]
>SET /DEF=[367,367]
>@AUTOIN
RSX-11M/M-PLUS Auto-Install Procedure V1.1
24-MAR-16 18:42:19
Type "?" for help; CTRL/Z to end; or valid input.
Which product(s) do you want to install? F77
Type "?" for help; CTRL/Z to exit Auto-Install; or valid input.
Where are the update files located ?
Type "?" for help; CTRL/Z to skip this product; or valid input.
Which device are the distribution files for F77 (F77) located on (include colon)
? MU1:
BRU - Starting Tape 1 on MU1:
BRU - End of Tape 1 on MU1:
BRU - Completed
Products being installed:
Device Product Task name
------ ------- ---------
MU1: F77 (F77)
Determining system configuration.
BRU - Starting Tape 1 on MU1:
BRU - End of Tape 1 on MU1:
BRU - Completed
WARNING -- no updates found for configuration data file; procedure continuing.
Do you want to customize F77 (F77) (Y/N) ?
Installation of F77 (F77) beginning at 24-MAR-16 18:44:39
Reading F77F77.CFG.
Transferring kit files to work area.
BRU - Starting Tape 1 on MU1:
BRU - End of Tape 1 on MU1:
BRU - Completed
BRU - Starting Tape 1 on MU1:
BRU - End of Tape 1 on MU1:
BRU - Completed
18:44:40 *** MU1: -- Dismount completeDMO -- TT0: dismounted from MU1: *** Final dismount initiated ***
Updating kit files.
Module "CMDUTI" replaced
Module "CODEX1" replaced
Module "IOBLKS" replaced
Module "$DATE " replaced
Module "$IDATE" replaced
Building product F77 (F77).
Running command procedure BLDTKB.CMD
Building product FORTRAN-77
BUILD FCS Version of the FORTRAN-77 OTS
Entry points deleted:
$ERTXT
BUILD RMS Version of the FORTRAN-77 OTS
Entry points deleted:
$ERTXT
Copying FORTRAN-77 FCS OTS to LB:[1,1]
Copying FORTRAN-77 RMS OTS to LB:[1,1]
Copy files to correct locations
FORTRAN-77 release notes
FORTRAN-77 message file
FORTRAN-77 compiler overlay descriptor file
FORTRAN-77 compiler TKB command file
FORTRAN-77 overlay descriptor file for the FCS OTS
FORTRAN-77 overlay descriptor file for the RMS OTS
FORTRAN-77 RSX-11S OTS
FORTRAN-77 alternate convert module
FORTRAN-77 extended instruction set module
FORTRAN-77 alternate error reporting module
FORTRAN-77 alternate I/O module
FORTRAN-77 alternate random number generator
FORTRAN-77 intrinsic mapping module
File for building OTS resident libraries and vector
File to exclude FORTRAN-77 OTS entry points
File used in building OTS resident library vector
Command file for building clustered FCS OTS
TKB command file for clustered FCS OTS
Clustered FCS OTS tailor file
Command file for building non-clustered FCS OTS
TKB command file for non-clustered FCS OTS
Non-clustered FCS OTS tailor file
Command file for FCS OTS linked against FCSFSL
TKB file for FCS OTS linking against FCSFSL
Tailor file for FCS OTS linked against FCSFSL
Command file for building clustered RMS OTS
TKB command file for clustered RMS OTS
Clustered RMS OTS tailor file
File needed to build FCS OTS resident libraries
Copying F77.TSK to LB:[3,54]F77.TSK
Transferring files from work area.
Running IVP command procedure F77IVP.CMD.
Test the compiler's ability to detect a compile time error
The following error should be seen:
F77 -- ERROR 28-E Overflow while converting constant or constant expression
[I = 71347] in module F77TST at line 6
F77 -- 1 Error F77TST.FTN;1
**************************** end of comment ********************************
F77 -- ERROR 28-E Overflow while converting constant or constant expression
[I = 71347] in module F77TST at line 6
F77 -- 1 Error F77TST.FTN;1
Task-build the test program
Test the ability of the OTS to detect the run-time error.
The following message should be displayed:
NNNNNN -- ERROR 73
Floating zero divide
at PC = xxxxxx
in "F77TST" at or after 6
Where NNNNNN is the task name and xxxxxx is the actual program location
**************************** end of comment ***************************
Testing the FCS version of the FORTRAN-77 OTS
TT0 -- ERROR 73
Floating zero divide
at PC = 001740
in "F77TST" at or after 6
PDP-11 FORTRAN-77 INSTALLATION SUCCESSFUL!
TT0 -- STOP
Testing the RMS version of the FORTRAN-77 OTS
TT0 -- ERROR 73
Floating zero divide
at PC = 044234
in "F77TST" at or after 6
PDP-11 FORTRAN-77 INSTALLATION SUCCESSFUL!
TT0 -- STOP
Purging old files
Installation of F77 (F77) ending at 24-MAR-16 18:44:46.
Installation of F77 (F77) successful.
Auto-Install ended on 24-MAR-16 at 18:44:46.
>
Готово! Ну и остается только прописать в STARTUP.CMD его загрузку:
.; FORTRAN77 v5.4
.IFNINS ...F77 INS $F77
комментарии # 01-09-2017 09:00, Unik

### Оставить комментарий к «FORTRAN-77 5.4»

Имя
Текст комментария *

# ~Digital PDP-11~

## Навигация

## Страницы

О сайте

## Поиск

## Ссылки

- jaqblog
- Soft&Manual
- BASIC PDP-11
- PDP-11 Nostalgia
- PDP-11
- Ancient Bits adventure
- pdp-11.org.ru
- RetroCMP
- Soft
- Soft and other
- PDP2011
- Raspberry Pi PDP-11
- RSX11M.com
- Paper Tape
- TU-58 XXDP
***
- RSTS/E
- ELVIRA
- Wofford WITCH
- RSTS.org
- RSTS/E walkthru

gopher://pdp11.tk/

## Комментарии

Korchagin в Turtles Ninja
Гость в Доступный PDP-11. Часть 2.
Vladimir в PDP-11/45 online