From: Digest <deadmail>
To: "OS/2GenAu Digest"<deadmail>
Date: Thu, 11 May 2006 00:00:28 EST-10EDT,10,-1,0,7200,3,-1,0,7200,3600
Subject: [os2genau_digest] No. 1294
Reply-To: <deadmail>
X-List-Unsubscribe: www.os2site.com/list/

**************************************************
Wednesday 10 May 2006
 Number  1294
**************************************************

Subjects for today
 
1  Re:  ECS 1.1 install problems (Becoming RSJ Updates) : Gavin Miller <gmi12896 at bigpond dot net dot au>
1  Re:  ECS 1.1 install problems (Becoming RSJ Updates) : Kev <kdownes at tpg dot com dot au>
2  Re:  PCI HOST CARD : nickl at pacific dot net dot au

**= Email   1 ==========================**

Date:  Wed, 10 May 2006 10:19:21 -0400
From:  Gavin Miller <gmi12896 at bigpond dot net dot au>
Subject:  Re:  ECS 1.1 install problems (Becoming RSJ Updates)

Hi Kev,

Yeah I had no idea about that.  So... no I'm not using BM since I didn't 
want to re partition things too much and other boot managers sit in the 
MBR without taking up too much space.

Now you might know this.  What are the rules for updating RSJ?

Cheers
G

Kev wrote:
> Gavin Miller wrote:
>> Problem solved.  Apologies to all for my rude outburst.  As it turned 
>> out, it didn't like the drive being called "d:".  Changed it to C: 
>> and no problems at all.
>
> I guess that answers my last question in my previous post on this 
> topic.  I'll bet you're not installing BM.  If you REALLY want D:, 
> install BM, set to automatically boot eCS in 1 second.  BM only takes 
> 7meg of disk space.
>
> Cheers
> Kev
>
----------------------------------------------------------------------------------
 

**= Email   1 ==========================**

Date:  Wed, 10 May 2006 12:10:50 +0800
From:  Kev <kdownes at tpg dot com dot au>
Subject:  Re:  ECS 1.1 install problems (Becoming RSJ Updates)

Gavin Miller wrote:

> Now you might know this.  What are the rules for updating RSJ?

All I ever did was install the new one over the old one.  The install 
script finds the old setup and does its thing from there.

Cheers
Kev

-- 
=========================
Kev Downes
kdownes at tpg dot com dot au  ph 0404 7 0808 2
We use and recommend Xandros 3.0.2
=========================
There are 10 types of people ...
    ... those who understand binary, and those who don't!
=========================
"Jesus Christ is the centre of everything and the object of everything;
He who does not know him, knows nothing of the order of the world
and nothing of himself."             Blaise Pascal
=========================
----------------------------------------------------------------------------------
 

**= Email   2 ==========================**

Date:  Wed, 10 May 2006 21:23:48 +0900
From:  nickl at pacific dot net dot au
Subject:  Re:  PCI HOST CARD

Hi All.

First of all, thank you for your posts. They have been most helpful, but
I'm still in a bit of a bind. <more>.

A friend of mine has donated one of these USB 2.0 to PCI Host Cards. Being
a Windows person, he didn't want to use it, as he had lost the
instructions to install. <G>.

Ironically, it is the Windows part that runs. It also can be seen on
Kubuntu Linux (but didn't want to open).

Here is what I sent to eComStation, as I'm using eCs2.0b2.

----------------------------------------------------------
A High Speed USB 2.0 PCI Host Card will not run under eCs2.0b2. Same card
runs under  Windows and Kubuntu Linux. Original USB with this Celeron 
P700 motherboard will run under 1.0, but the USB Pen Drive, when changed
from there to  the USB 2.0 will not run. USB Device Manager in Utilities
programme does not detect the Pen Drive. Are latest USB Drivers being used
on eCs2.0b2? ----------------------------------------------------------

That would be my first question. Maybe a more elderly version of the USB
drivers run on eCs2.0b2 (for stability reasons, whilst other sections of
the OS is being tested?). What is a quick way I could test for that? I
have also suddenly realised that the snippet of CONFIG.SYS I sent was from
my system (that I'm writing from now) which is running eCs1.2MR
(downloaded version) and sorted under Doug Bissett's system, and not
eCs2.0b2 which uses a different sort method, and the USB Drivers are
spread out.

Which brings another question: I have heard that there should be separate
entrys for each USB ports in CONFIG.SYS. Two things makes me wonder:
Firstly, the 2xUSB 1.0 ports that come up with the motherboard work
alright....it's the 4x new ones on the PCI Card that do not. Secondly:
Which entry(ies) do I have to repeat, and Thirdly: I thought sending
/REMOVABLES:2 to REMOVABLES:6 would solve that. Maybe not, but then maybe
I have the wrong USB Version in.

Or maybe, just maybe, I'm missing something really simple. Apologies for
bothering you all again, but any ideas would be greatly appreciated.

Looking forward to hearing from you.

Regards

NICK

In <200605040529.k445TN2o031153 at mailproxy1.pacific dot net dot au>, on 05/04/2006 
   at 01:13 PM, nickl at pacific dot net dot au said:

>Hi All.

>Has there been a posting on PCI Host Cards working with eCs-OS/2?

>I saw one in the shop the other day, and as I have USB1.2, it seems like
>an answer....at least until I saw the wintendo drivers required.

>I asked what drivers. The Sales Assistant did not know, but I worked out
>that they could mean USB Drivers....maybe rather similar to what I have
>in my CONFIG.SYS, as shown here:

>REM [USB section
>BASEDEV=USBUHCD.SYS
>BASEDEV=USBUHCD.SYS
>BASEDEV=USBD.SYS
>BASEDEV=USBHID.SYS
>DEVICE=E:\OS2\BOOT\USBPRT.SYS
>REM DEVICE=E:\OS2\BOOT\USBMOUSE.SYS
>REM DEVICE=E:\OS2\BOOT\USBKBD.SYS
>DEVICE=E:\ECS\BOOT\USBRESMG.SYS
>BASEDEV=USBMSD.ADD /FLOPPIES:0 /REMOVABLES:4 /v

>Has anybody had success with these cards? Was there major surgery
>required to the above entries on order to make it work for eCs-OS/2?

>Look forward to, and thanks in advance to your answers.

>Regards

>NICK

>-----------------------------------------------------------
>nickl at pacific dot net dot au
>-----------------------------------------------------------


> 


-----------------------------------------------------------
nickl at pacific dot net dot au
-----------------------------------------------------------

----------------------------------------------------------------------------------
 

