From: Digest <deadmail>
To: "OS/2GenAu Digest"<deadmail>
Date: Fri, 23 Jan 2004 00:01:03 EST-10EDT,10,-1,0,7200,3,-1,0,7200,3600
Subject: [os2genau_digest] No. 782
Reply-To: <deadmail>
X-List-Unsubscribe: www.os2site.com/list/

**************************************************
Thursday 22 January 2004
 Number  782
**************************************************

Subjects for today
 
1   AC'97 Sound and VIA Rhine II Fast Ethernet : k.downes at optusnet dot com dot au
2  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : brianb at kdfisher dot com dot au
3  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : brianb at kdfisher dot com dot au
4  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : k.downes at optusnet dot com dot au
5  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : k.downes at optusnet dot com dot au
6  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : k.downes at optusnet dot com dot au
7  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : brianb at kdfisher dot com dot au
8  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet : Mark Dodel" <madodel at ptdprolog dot net>
9   Loooooking for a SCSI scanner : John Angelico" <talldad at kepl dot com dot au>
10   p3 m/b ac97 audio driver ? : voytek at sbt dot net dot au
11  Re:  Loooooking for a SCSI scanner : Ed Durrant <edurrant at bigpond dot net dot au>
12   VIA ethernet card : k.downes at optusnet dot com dot au
13   eCS MT : k.downes at optusnet dot com dot au
14  Re:  p3 m/b ac97 audio driver ? : Robert Traynor  (BobT)" <rtraynor at optusnet dot com dot au>
15  Re:  p3 m/b ac97 audio driver ? : voytek at sbt dot net dot au
16  Re:  VIA ethernet card : Mike O'Connor <mikeoc at dodo dot com dot au>
17  Re:  eCS MT : Mike O'Connor <mikeoc at dodo dot com dot au>
18  Re:  eCS MT : Mike O'Connor <mikeoc at dodo dot com dot au>
19  Re:  p3 m/b ac97 audio driver ? : Mike O'Connor <mikeoc at dodo dot com dot au>
20  Re:  Loooooking for a SCSI scanner : John Angelico" <talldad at kepl dot com dot au>

**= Email   1 ==========================**

Date:  Wed, 21 Jan 2004 22:05:02 +0800
From:  k.downes at optusnet dot com dot au
Subject:   AC'97 Sound and VIA Rhine II Fast Ethernet

Hi all.  I've been persevering, but not with a great deal of success.

I've recently come by an MSI KM2M Combo Series motherboard and an AMD
Athlon XP2000+ processor.  I have most of it working except 2 things ...

1. Does anyone know of any drivers which will work with an AC'97 sound
card based on a Realtek ALC650 codec on a motherboard with a VIA KM266
chipset and a VIA VT8235 chipset?  I don't know what most of that means -
I've taken it from the motherboard handbook.  The best I can see so far
are drivers which will work with the Realtek ALC650 codec on a motherboard
with an Intel chipset.  These drivers cause a trap on my system.

2. The LAN card is a VIA Rhine II Fast Ethernet Adapter.  I have it
working (sort of) with some VIA drivers I found via the Nicdetc.CMD
utility.  The book says I have, "VIA VT8235 integrated MAC + VIA 6103
PHY".  It only runs at 10 Mbits.

I'd really like to know if I can these 2 services working properly.

Thanx in advance
Kev Downes
=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------
 

**= Email   2 ==========================**

Date:  Thu, 22 Jan 2004 10:44:51 +0930
From:  brianb at kdfisher dot com dot au
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet


Kev,
I have a driver for the ACL650. From memory I
got it from the RealTek web site.

If you cant track it down let me know and I will
e-mail it to you off the list.

-----------------------------------------
Brian Butler
System Administrator
brianb at kdfisher dot com dot au


                                                                                                                                
                      k.downes at optusnet                                                                                         
                       dot com dot au                  To:       os2genau at os2 dot org dot au                                                    
                                               cc:                                                                              
                      22/01/2004 00:35         Subject:   AC'97 Sound and VIA Rhine II Fast Ethernet                  
                      Please respond to                                                                                         
                      os2genau                                                                                                  
                                                                                                                                
                                                                                                                                




Hi all.  I've been persevering, but not with a great deal of success.

I've recently come by an MSI KM2M Combo Series motherboard and an AMD
Athlon XP2000+ processor.  I have most of it working except 2 things ...

1. Does anyone know of any drivers which will work with an AC'97 sound
card based on a Realtek ALC650 codec on a motherboard with a VIA KM266
chipset and a VIA VT8235 chipset?  I don't know what most of that means -
I've taken it from the motherboard handbook.  The best I can see so far
are drivers which will work with the Realtek ALC650 codec on a motherboard
with an Intel chipset.  These drivers cause a trap on my system.

2. The LAN card is a VIA Rhine II Fast Ethernet Adapter.  I have it
working (sort of) with some VIA drivers I found via the Nicdetc.CMD
utility.  The book says I have, "VIA VT8235 integrated MAC + VIA 6103
PHY".  It only runs at 10 Mbits.

I'd really like to know if I can these 2 services working properly.

Thanx in advance
Kev Downes
=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------

 






----------------------------------------------------------------------------------
 

**= Email   3 ==========================**

Date:  Thu, 22 Jan 2004 11:03:36 +0930
From:  brianb at kdfisher dot com dot au
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet


Kev,
If your NIC is a DLink DFE530-TX then I also have an
OS/2 driver for it.
Can't recall where I found that so let me know if
you want to give it a try and I will send it to you
off list.

As for the 10mb only problem I found the DFE530
does not auto negotiate well. Try forcing it to 100mb
in the protocol.ini file.

-----------------------------------------
Brian Butler
System Administrator
brianb at kdfisher dot com dot au


                                                                                                                                
                      k.downes at optusnet                                                                                         
                       dot com dot au                  To:       os2genau at os2 dot org dot au                                                    
                                               cc:                                                                              
                      22/01/2004 00:35         Subject:   AC'97 Sound and VIA Rhine II Fast Ethernet                  
                      Please respond to                                                                                         
                      os2genau                                                                                                  
                                                                                                                                
                                                                                                                                




Hi all.  I've been persevering, but not with a great deal of success.

I've recently come by an MSI KM2M Combo Series motherboard and an AMD
Athlon XP2000+ processor.  I have most of it working except 2 things ...

1. Does anyone know of any drivers which will work with an AC'97 sound
card based on a Realtek ALC650 codec on a motherboard with a VIA KM266
chipset and a VIA VT8235 chipset?  I don't know what most of that means -
I've taken it from the motherboard handbook.  The best I can see so far
are drivers which will work with the Realtek ALC650 codec on a motherboard
with an Intel chipset.  These drivers cause a trap on my system.

2. The LAN card is a VIA Rhine II Fast Ethernet Adapter.  I have it
working (sort of) with some VIA drivers I found via the Nicdetc.CMD
utility.  The book says I have, "VIA VT8235 integrated MAC + VIA 6103
PHY".  It only runs at 10 Mbits.

I'd really like to know if I can these 2 services working properly.

Thanx in advance
Kev Downes
=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------

 






----------------------------------------------------------------------------------
 

**= Email   4 ==========================**

Date:  Thu, 22 Jan 2004 08:37:49 +0800
From:  k.downes at optusnet dot com dot au
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet

Hi Brian, thanx for your response.  I have just dnloaded the sound driver
- thanx!  As for the LAN driver I haven't seen "DLink" mentioned anywhere
in the m/b book so I assume that it is in fact a VIA LAN chipset. 
Whatever it is it's built into the m/b.

Thanx again
Kev Downes


In <OFF1CFD050.4B27B9E4-ON69256E23.000848EB at kdfisher dot com dot au>, on
01/22/2004 
   at 11:03 AM, brianb at kdfisher dot com dot au said:


>Kev,
>If your NIC is a DLink DFE530-TX then I also have an
>OS/2 driver for it.
>Can't recall where I found that so let me know if
>you want to give it a try and I will send it to you
>off list.

>As for the 10mb only problem I found the DFE530
>does not auto negotiate well. Try forcing it to 100mb
>in the protocol.ini file.

>-----------------------------------------
>Brian Butler
>System Administrator
>brianb at kdfisher dot com dot au


>                                                                                                                                
>                      k.downes at optusnet                                                                                        

>                       dot com dot au                  To:      
>os2genau at os2 dot org dot au                                                    
>                                               cc:                                                                             

>                      22/01/2004 00:35         Subject:   AC'97
>Sound and VIA Rhine II Fast Ethernet                  
>                      Please respond to                                                                                        

>                      os2genau                                                                                                 

>                                                                                                                                
>                                                                                                                                




>Hi all.  I've been persevering, but not with a great deal of success.

>I've recently come by an MSI KM2M Combo Series motherboard and an AMD
>Athlon XP2000+ processor.  I have most of it working except 2 things ...

>1. Does anyone know of any drivers which will work with an AC'97 sound
>card based on a Realtek ALC650 codec on a motherboard with a VIA KM266
>chipset and a VIA VT8235 chipset?  I don't know what most of that means -
>I've taken it from the motherboard handbook.  The best I can see so far
>are drivers which will work with the Realtek ALC650 codec on a
>motherboard with an Intel chipset.  These drivers cause a trap on my
>system.

>2. The LAN card is a VIA Rhine II Fast Ethernet Adapter.  I have it
>working (sort of) with some VIA drivers I found via the Nicdetc.CMD
>utility.  The book says I have, "VIA VT8235 integrated MAC + VIA 6103
>PHY".  It only runs at 10 Mbits.

>I'd really like to know if I can these 2 services working properly.

>Thanx in advance
>Kev Downes
=========================
>k.downes at optusnet dot com dot au
>Windows is not the answer. Windows is the question. The answer is NO!  
>We use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
>"Jesus Christ is the centre of everything and the object of everything;
>and he who does not know him, knows nothing of the order of the world and
>nothing of himself."             Blaise Pascal
=========================



> 







> 


=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------
 

**= Email   5 ==========================**

Date:  Thu, 22 Jan 2004 09:04:46 +0800
From:  k.downes at optusnet dot com dot au
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet

In <OFF1CFD050.4B27B9E4-ON69256E23.000848EB at kdfisher dot com dot au>, on
01/22/2004 
   at 11:03 AM, brianb at kdfisher dot com dot au said:


>As for the 10mb only problem I found the DFE530
>does not auto negotiate well. Try forcing it to 100mb
>in the protocol.ini file.


Hi brian.  Wrt the above, I went for a look in my PROTOCOL.INI and have no
clues what to to do.  Below is a copy of the file.  Is it possible for you
to show me what to do?

Thanx 
Kev Downes
=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------
 

**= Email   6 ==========================**

Date:  Thu, 22 Jan 2004 09:07:25 +0800
From:  k.downes at optusnet dot com dot au
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet

In <OFF1CFD050.4B27B9E4-ON69256E23.000848EB at kdfisher dot com dot au>, on
01/22/2004 
   at 11:03 AM, brianb at kdfisher dot com dot au said:


>As for the 10mb only problem I found the DFE530
>does not auto negotiate well. Try forcing it to 100mb
>in the protocol.ini file.


Hi brian.  Wrt the above, I went for a look in my PROTOCOL.INI and have no
clues what to to do.  Below is a copy of the file.  Is it possible for you
to show me what to do?

Thanx 
Kev Downes

[PROT_MAN]

   DRIVERNAME = PROTMAN$

[IBMLXCFG]

   netbeui_nif = netbeui.nif
   tcpip_nif = tcpip.nif
   FETND_nif = FETND.nif

[NETBIOS]

   DriverName = netbios$
   ADAPTER0 = netbeui$,0

[netbeui_nif]

   DriverName = netbeui$
   Bindings = FETND_nif
   ETHERAND_TYPE = "I"
   USEADDRREV = "YES"
   OS2TRACEMASK = 0x0
   SESSIONS = 130
   NCBS = 225
   NAMES = 21
   SELECTORS = 50
   USEMAXDATAGRAM = "NO"
   ADAPTRATE = 1000
   WINDOWERRORS = 0
   MAXDATARCV = 4168
   TI = 30000
   T1 = 1000
   T2 = 200
   MAXIN = 1
   MAXOUT = 1
   NETBIOSTIMEOUT = 500
   NETBIOSRETRIES = 3
   NAMECACHE = 1000
   RNDOPTION = 1
   PIGGYBACKACKS = 1
   DATAGRAMPACKETS = 50
   PACKETS = 300
   LOOPPACKETS = 8
   PIPELINE = 5
   MAXTRANSMITS = 6
   MINTRANSMITS = 2
   DLCRETRIES = 10
   FCPRIORITY = 5
   NETFLAGS = 0x0

[tcpip_nif]

   DriverName = TCPIP$
   Bindings = FETND_nif

[FETND_nif]

   DriverName = FETND$
   CONNECTIONTYPE = "AUTOSENSE"
   FLOW_CONTROL = "Hardware_Default"



=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------
 

**= Email   7 ==========================**

Date:  Thu, 22 Jan 2004 11:55:45 +0930
From:  brianb at kdfisher dot com dot au
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet


Kev,
The section you need to edit is at the end of the file.

[FETND_nif]

   DriverName = FETND$
   CONNECTIONTYPE = "AUTOSENSE"
   FLOW_CONTROL = "Hardware_Default"

The CONNECTIONTYPE parameter is the one
the sets link speed.

The following is from the notes with the D-Link driver
As I don't know whether your Ethernet is full duplex or not
I can only say try each of the 100mb options. Full duplex is
better if the rest of your Ethernet hardware is using it.

NOTE the leading underscore!

Save a backup copy of the original file before you tamper with it!

If you get it wrong OS/2 will still boot but it will give you errors
at startup about not loading the Ethernet driver if there is something
it does not like in the INI file.

; CONNECTIONTYPE = AUTOSENSE
;   AUTOSENSE             ;Auto-select media type and line speed
;   _10BASET              ;Force the driver to select 10Mbps half duplex
mode.
;   _10BASETFD            ;Force the driver to select 10Mbps full duplex
mode.
;   _100BASETX            ;Force the driver to select 100Mbps half duplex
mode.
;   _100BASETXFD          ;Force the driver to select 100Mbps full duplex
mode.
;
;
;   Keywords supported by DLKFET
;
;     AUTOSENSE       - This keyword performs power-up autosense on all
;                       types of boards in order to connect to the active
;                       line, and dynamic media autosensing (at run-time)
;                       on boards supporting it. Without specifying any
;                       keyword this one will be used as default one.
;
;     _10BASET         - This keyword force media type to be 10Mbps half
;                       duplex, and disable power-up autosense.
;
;     _10BASETFD       - This keyword force media type to be 10Mbps full
;                       duplex, and disable power-up autosense.
;
;     _100BASETX       - This keyword force media type to be 100Mbps half
;                       duplex, and disable power-up autosense.
;
;     _100BASETXFD     - This keyword force media type to be 100Mbps full
;                       duplex, and disable power-up autosense.


-----------------------------------------
Brian Butler
System Administrator
brianb at kdfisher dot com dot au


----------------------------------------------------------------------------------
 

**= Email   8 ==========================**

Date:  Wed, 21 Jan 2004 22:42:06 -0500
From:  "Mark Dodel" <madodel at ptdprolog dot net>
Subject:  Re:  AC'97 Sound and VIA Rhine II Fast Ethernet

In <200401220002.i0M02Y723174 at mail017.syd.optusnet dot com dot au>, on 01/21/04 at
10:05 PM,
   k.downes at optusnet dot com dot au said:

>1. Does anyone know of any drivers which will work with an AC'97 sound
>card based on a Realtek ALC650 codec on a motherboard with a VIA KM266
>chipset and a VIA VT8235 chipset?  I don't know what most of that means -
>I've taken it from the motherboard handbook.  The best I can see so far
>are drivers which will work with the Realtek ALC650 codec on a
>motherboard with an Intel chipset.  These drivers cause a trap on my
>system.

Besides the Realtek driver for the ALC650, which has been known to have
problems with shared resources (IRQs), the UNIAUD driver will also work
with that chipset.  

Realtek ALC driver: 
<http://www.realtek dot com.tw/downloads/dlac97-2.aspx?lineid=5&famid=12&series=8&Software=True>

UNIAUD: <http://os2.kiev.ua/> (Not sure of the exact URL as right now I
can't get to their web site, but its probably something like
http://os2.kiev.ua/en/uniaud.php )

I have an ALC201 which works OK with the latest UNIAUD driver, but not at
all with the Realtek.


Mark

-- 

 From the eComStation Desktop of: Mark Dodel

  Warpstock 2003 - See the video and presentations: http://www.warpstock dot org

For a choice in the future of personal computing, Join VOICE - http://www.os2voice dot org

  "The liberty of a democracy is not safe if the people tolerate the growth of private power to a point where it becomes stronger than their democratic State itself.   That in it's essence, is Fascism - ownership of government by an individual, by a group or by any controlling private power." Franklin Delano Roosevelt, Message proposing the Monopoly Investigation, 1938 


----------------------------------------------------------------------------------
 

**= Email   9 ==========================**

Date:  Thu, 22 Jan 2004 15:49:48 +1100 (AEDT)
From:  "John Angelico" <talldad at kepl dot com dot au>
Subject:   Loooooking for a SCSI scanner

Hi all!

We are looking for a scanner which fulfills the following specs:
- SCSI 
- flat-bed
- suitable for reasonably high resolution work - photos as well as text
- OS/2-eCS support (usually Tame/SANE)
- working (<g> we have gotten tired of fiddling with cables and cards)
- plug/n/go

Advice please.

Pointers to potential sellers, please.


Best regards
John Angelico
OS/2 SIG
os2 at melbpc dot org dot au or 
talldad at kepl dot com dot au
___________________

PMTagline v1.50 - Copyright, 1996-1997, Stephen Berg and John Angelico
.... Those who refuse to learn from the past are condemned to repeat it.
----------------------------------------------------------------------------------
 

**= Email   10 ==========================**

Date:  Thu, 22 Jan 2004 20:54:15 +1100 (EST)
From:  voytek at sbt dot net dot au
Subject:   p3 m/b ac97 audio driver ?

I have a P3 m/b with an AC97 Audio chipset, is there any possibly of
getting an OS/2 driver for it ?

it also has a AC97 modem, is that a win modem thingo ?

as there is nor RJ jack, I guess, it needs some daughter board ? into an
empty mb/ slot ?


----------------------------------------------------------------------------------
 
**= Email   11 ==========================**

Date:  Thu, 22 Jan 2004 21:03:20 +1100
From:  Ed Durrant <edurrant at bigpond dot net dot au>
Subject:  Re:  Loooooking for a SCSI scanner

I use a Canon FB620S with very good results and reliability with TAME.

As per usual technology is ever changing and I don't think this model is still
available new (try eBAY?),
but the following models are current and I'm pretty sure we should be able to make
SANE/TAME work with them:

http://www.canon dot com dot au/products/scanners/scanners_low_medium_volume.html

Cheers/2

Ed.

John Angelico wrote:

> Hi all!
>
> We are looking for a scanner which fulfills the following specs:
> - SCSI
> - flat-bed
> - suitable for reasonably high resolution work - photos as well as text
> - OS/2-eCS support (usually Tame/SANE)
> - working (<g> we have gotten tired of fiddling with cables and cards)
> - plug/n/go
>
> Advice please.
>
> Pointers to potential sellers, please.
>
> Best regards
> John Angelico
> OS/2 SIG
> os2 at melbpc dot org dot au or
> talldad at kepl dot com dot au
> ___________________
>
> PMTagline v1.50 - Copyright, 1996-1997, Stephen Berg and John Angelico
> ... Those who refuse to learn from the past are condemned to repeat it.

>  


----------------------------------------------------------------------------------
 

**= Email   12 ==========================**

Date:  Thu, 22 Jan 2004 17:51:46 +0800
From:  k.downes at optusnet dot com dot au
Subject:   VIA ethernet card

Help Please!!

As stated in an earlier message, I recently came by an MSI KM2M Combo
Series motherboard and an AMD Athlon XP2000+ processor.  I have most of it
working now except this ...

The LAN card (on the motherboard) is a VIA Rhine II Fast Ethernet Adapter.
 I have it working (sort of) with some VIA drivers I found via the
Nicdetc.CMD utility.  The book says I have, "VIA VT8235 integrated MAC +
VIA 6103 PHY".  This is what the driver reports during boot up ...

    VIA PCI 10/100 Mb Fast Ethernet Adapter
    NDIS OS/2 Driver V3.18(04-12-2001)

    Flow Control is Hardware Default
            Interrupt = 0xB
            IOBase    = 0xB800
    Half Duplex, Linespeed = 10 Ethernet Address:
                        000C766B1D31 Slot(HEX): 0

I suspect that it isn't running its best!  Brian Butler has responded with
some info to help me edit my PROTOCOL.INI, but I'm too ignorant to
understand exactly what he said.  I'm unable to relate his suggested edits
to my PROTOCOL.INI.  Below is my PROTOCOL.INI.  Btw, I *do* appreciate
your help Brian, but I'm just too dumb to grasp it.  I suspect that I
don't have a DLink card in disguise.

Thanx in advance
Kev Downes

[PROT_MAN]

   DRIVERNAME = PROTMAN$

[IBMLXCFG]

   netbeui_nif = netbeui.nif
   tcpip_nif = tcpip.nif
   FETND_nif = FETND.nif

[NETBIOS]

   DriverName = netbios$
   ADAPTER0 = netbeui$,0

[netbeui_nif]

   DriverName = netbeui$
   Bindings = FETND_nif
   ETHERAND_TYPE = "I"
   USEADDRREV = "YES"
   OS2TRACEMASK = 0x0
   SESSIONS = 130
   NCBS = 225
   NAMES = 21
   SELECTORS = 50
   USEMAXDATAGRAM = "NO"
   ADAPTRATE = 1000
   WINDOWERRORS = 0
   MAXDATARCV = 4168
   TI = 30000
   T1 = 1000
   T2 = 200
   MAXIN = 1
   MAXOUT = 1
   NETBIOSTIMEOUT = 500
   NETBIOSRETRIES = 3
   NAMECACHE = 1000
   RNDOPTION = 1
   PIGGYBACKACKS = 1
   DATAGRAMPACKETS = 50
   PACKETS = 300
   LOOPPACKETS = 8
   PIPELINE = 5
   MAXTRANSMITS = 6
   MINTRANSMITS = 2
   DLCRETRIES = 10
   FCPRIORITY = 5
   NETFLAGS = 0x0

[tcpip_nif]

   DriverName = TCPIP$
   Bindings = FETND_nif

[FETND_nif]

   DriverName = FETND$
   CONNECTIONTYPE = "AUTOSENSE"
   FLOW_CONTROL = "Hardware_Default"






=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------
 

**= Email   13 ==========================**

Date:  Thu, 22 Jan 2004 18:13:40 +0800
From:  k.downes at optusnet dot com dot au
Subject:   eCS MT

Hope you gize can bear with me while I sort out a few things.  I've been
installing eCS1.1 (several times) in an attempt to get what I want.  I
have a barely acceptable install now, and have just installed eCS
Maintenance Tool (v 2.1.5.9) and I allowed it to install into its default
directory (E:\ecs\system\ECSMT200).  The same directory was set (by
default) as the download path and fix path.

I already have downloaded many of the fixes, including fixpak 4, which I
don't want to have to download again (I'm on dial-up), so I copied them
all to the download path.

My question is, how do I make ECS MT see the files which I already have,
so that I can apply the fixes?  (I do hate that ECS MT!  I just wasn't
made for normal people to use)

Thanx again gize
Kev Downes
=========================
k.downes at optusnet dot com dot au
Windows is not the answer. Windows is the question. The answer is NO!   We
use and recommend IBM OS/2 Warp and Serenity System's eComStation.
=========================
"Jesus Christ is the centre of everything and the object of everything;
and he who does not know him, knows nothing of the order of the world and
nothing of himself."             Blaise Pascal
=========================

----------------------------------------------------------------------------------
 

**= Email   14 ==========================**

Date:  Thu, 22 Jan 2004 22:08:41 +1000
From:  "Robert Traynor  (BobT)" <rtraynor at optusnet dot com dot au>
Subject:  Re:  p3 m/b ac97 audio driver ?

Hi Voytek,

I don't know if this will help.
Answers below.


On Thu, 22 Jan 2004 20:54:15 +1100 (EST), voytek at sbt dot net dot au wrote:
> I have a P3 m/b with an AC97 Audio chipset, is there any possibly of
> getting an OS/2 driver for it ?

You have not stated the chipset nor the motherboard.  
If it is a SoundMax chipset then check out the SoundMax driver on hobbes.
Just search for SoundMax as one word.

If not then try the Uniaud drivers.

My P4 Asus P4c-800 is currently working fine with the hobbes
SoundMax driver.  


> it also has a AC97 modem, is that a win modem thingo ?
> as there is nor RJ jack, I guess, it needs some daughter board ? into an
> empty mb/ slot ?

You probably need a riser card and it is probably a WinModem.


Regards,
Robert Traynor (BobT).
22 January 2004   22:04


   ,-._|\       Robert Traynor        (BobT)
 /  Oz  \      email            rtraynor at removeme.optusnet dot com dot au
 \_,--.x/ 


----------------------------------------------------------------------------------
 

**= Email   15 ==========================**

Date:  Thu, 22 Jan 2004 22:34:18 +1100 (EST)
From:  voytek at sbt dot net dot au
Subject:  Re:  p3 m/b ac97 audio driver ?

thanks, Bob

> You have not stated the chipset nor the motherboard.
> If it is a SoundMax chipset then check out the SoundMax driver on hobbes.
> Just search for SoundMax as one word.
>
> If not then try the Uniaud drivers.
>
> My P4 Asus P4c-800 is currently working fine with the hobbes
> SoundMax driver.

it's an Asus PC & Asus m/b (?)

is there any way to query the chipset , or do I need to get the torch and
screwdriver out ?
----------------------------------------------------------------------------------
 
**= Email   16 ==========================**

Date:  Thu, 22 Jan 2004 21:36:28 +1000
From:  Mike O'Connor <mikeoc at dodo dot com dot au>
Subject:  Re:  VIA ethernet card

k.downes at optusnet dot com dot au wrote:

><SNIPPED>
>

>This is what the driver reports during boot up ...
>
>    VIA PCI 10/100 Mb Fast Ethernet Adapter
>*    Half Duplex, Linespeed = 10 Ethernet Address:
>
[This means the cable is not supporting full-duplex]

>[FETND_nif]
>
>   DriverName = FETND$
>******   CONNECTIONTYPE = "AUTOSENSE"  ******
>   FLOW_CONTROL = "Hardware_Default"
>  
>

Hi Kev,
Unfortunately, I didn't keep Brian's response to you, I thought that was 
now cleared up, but I guess you've still retained it.

Where you have the line :

CONNECTIONTYPE = "AUTOSENSE" above, at the end of protocol.ini

change this to read:

CONNECTIONTYPE = "_100??????"


i.e. the one without the "D" for duplex - Brian quoted the entries for 
10 & 100 mbps for full-duplex [the ones ending with a 'D'] and ditto for 
the half-duplex settings [without the D]. you have to force the system 
to recognise that it's a 100mbps connection by specifying the entry that 
starts with _100.  just do the edit [with e.exe] and then save the 
protocol.ini.

HTH

-- 
Regards,
Mike

Failed the exam for
--------------------
MCSE - Minesweeper Consultant and Solitaire Expert
--------------------
[ISP blocks *.exe attachments]
[Please use zipped versions of above]



----------------------------------------------------------------------------------
 

**= Email   17 ==========================**

Date:  Thu, 22 Jan 2004 21:20:13 +1000
From:  Mike O'Connor <mikeoc at dodo dot com dot au>
Subject:  Re:  eCS MT

k.downes at optusnet dot com dot au wrote:

>Hope you gize can bear with me while I sort out a few things.  I've been
>installing eCS1.1 (several times) in an attempt to get what I want.  I
>have a barely acceptable install now, and have just installed eCS
>Maintenance Tool (v 2.1.5.9) and I allowed it to install into its default
>directory (E:\ecs\system\ECSMT200).  The same directory was set (by
>default) as the download path and fix path.
>
>I already have downloaded many of the fixes, including fixpak 4, which I
>don't want to have to download again (I'm on dial-up), so I copied them
>all to the download path.
>
>My question is, how do I make ECS MT see the files which I already have,
>so that I can apply the fixes?  (I do hate that ECS MT!  I just wasn't
>made for normal people to use)
>
>Thanx again gize
>Kev Downes
>  
>
Hi Kev,
In your Browser, or newsreader if you have one, and get subscribed to 
the ecomstation.support.ecsmt NG and as many of the others like 
ecomstation.support.install as you like at < news.ecomstation.nl > or < 
news.ecomstation dot com >.  You'll find out what everyone else did in 
similar/identical circumstances.

Your very question about using stuff you've already downloaded came up 
on the ecomstation group Yahoo list in the past couple of days and Chuck 
McKinnis, the former IBM'er who developed eCSMT was the one replying.

To subscribe automatically, send an e-mail with subject of "subscribe" 
to < eComStation-usubscribe at yahoogroups dot com >, and you'll get the 
information on how to join up.  It's pretty painless, once you have a 
Yahoo ID, and that *doesn't* mean you'll get spammed.

HTH

-- 
Regards,
Mike

Failed the exam for
--------------------
MCSE - Minesweeper Consultant and Solitaire Expert
--------------------
[ISP blocks *.exe attachments]
[Please use zipped versions of above]



----------------------------------------------------------------------------------
 

**= Email   18 ==========================**

Date:  Thu, 22 Jan 2004 21:46:42 +1000
From:  Mike O'Connor <mikeoc at dodo dot com dot au>
Subject:  Re:  eCS MT

Mike O'Connor wrote:

> k.downes at optusnet dot com dot au wrote:
>
>> Hope you gize can bear with me while I sort out a few things.  I've been
>> installing eCS1.1 (several times) in an attempt to get what I want.  I
>> have a barely acceptable install now, and have just installed eCS
>> Maintenance Tool (v 2.1.5.9) and I allowed it to install into its 
>> default
>> directory (E:\ecs\system\ECSMT200).  The same directory was set (by
>> default) as the download path and fix path.
>>
>> I already have downloaded many of the fixes, including fixpak 4, which I
>> don't want to have to download again (I'm on dial-up), so I copied them
>> all to the download path.
>>
>> My question is, how do I make ECS MT see the files which I already have,
>> so that I can apply the fixes?  (I do hate that ECS MT!  I just wasn't
>> made for normal people to use)
>>
>> Thanx again gize
>> Kev Downes
>>  
>>
> Hi Kev,
> Use your Browser, or newsreader if you have one, and get yourself 
> subscribed to the ecomstation.support.ecsmt NG and as many of the 
> others like ecomstation.support.install as you like at < 
> news.ecomstation.nl > or < news.ecomstation dot com >.  You'll find out 
> what everyone else did in similar/identical circumstances.
>
> Your very question about using stuff you've already downloaded came up 
> on the ecomstation group Yahoo list in the past couple of days and 
> Chuck McKinnis, the former IBM'er who developed eCSMT was the one 
> replying.
>
> To subscribe automatically, send an e-mail with subject of "subscribe" 
> to  < eComStation-subscribe at yahoogroups dot com >, and you'll get the 
> information on how to join up.  It's pretty painless, once you have a 
> Yahoo ID, and that *doesn't* mean you'll get spammed.
>
> HTH
>
Hi Kev,
TYPOs! :-[       usubscribe >> subscribe etc.,  now fixed in above!

-- 
Regards,
Mike

Failed the exam for
--------------------
MCSE - Minesweeper Consultant and Solitaire Expert
--------------------


[ISP blocks *.exe attachments]
[Please use zipped versions of above]



----------------------------------------------------------------------------------
 

**= Email   19 ==========================**

Date:  Thu, 22 Jan 2004 21:51:50 +1000
From:  Mike O'Connor <mikeoc at dodo dot com dot au>
Subject:  Re:  p3 m/b ac97 audio driver ?

voytek at sbt dot net dot au wrote:

>thanks, Bob
>
>>You have not stated the chipset nor the motherboard.
>>If it is a SoundMax chipset then check out the SoundMax driver on hobbes.
>>Just search for SoundMax as one word.
>>
>>If not then try the Uniaud drivers.
>>
>>My P4 Asus P4c-800 is currently working fine with the hobbes
>>SoundMax driver.
>>    
>>
>
>it's an Asus PC & Asus m/b (?)
>
>is there any way to query the chipset , or do I need to get the torch and
>screwdriver out ?
>

Hi Voytek,

Get hold of PCI048VK.zip on hobbes or Ian's www.os2site dot com.  Run the 
pci.exe in it and it will pump out everything you need to know and 
more.  You'll need to pipe it out to a file.

-- 
Regards,
Mike

Failed the exam for
--------------------
MCSE - Minesweeper Consultant and Solitaire Expert
--------------------
[ISP blocks *.exe attachments]
[Please use zipped versions of above]


----------------------------------------------------------------------------------
 

**= Email   20 ==========================**

Date:  Thu, 22 Jan 2004 23:50:39 +1100 (AEDT)
From:  "John Angelico" <talldad at kepl dot com dot au>
Subject:  Re:  Loooooking for a SCSI scanner

On Thu, 22 Jan 2004 21:03:20 +1100, Ed Durrant wrote:

>I use a Canon FB620S with very good results and reliability with TAME.

SCSI?

>
>As per usual technology is ever changing and I don't think this model is still
>available new (try eBAY?),
>but the following models are current and I'm pretty sure we should be able to make
>SANE/TAME work with them:
>
>http://www.canon dot com dot au/products/scanners/scanners_low_medium_volume.html

I saw some of those LiDE models in Officeworks today - all USB only.


Best regards
John Angelico
OS/2 SIG
os2 at melbpc dot org dot au or 
talldad at kepl dot com dot au
___________________

----------------------------------------------------------------------------------
 

