Date: Sun, 1 Apr 2001 01:00:40 +1100 (EDT)
Subject:   No.17

Date:- 01 April 2001

1================================================

From: "Gavin Miller" <paxtonatiaa dot com dot au>
Date: Sat, 31 Mar 2001 10:01:59 +1000 (EST)
Subject: Re: [os2genau] CD Audio playing problem

Hi Ed,

Try downloading the driver again if it keeps locking up at the end stages.  Sometimes the files can be 
corrupted just enough to do that sort of thing by noise in the lines or whatever.  I've had to do that once or 
twice.

Cheers.

2================================================

Date: Sat, 31 Mar 2001 15:15:34 -0500
From: Ed Durrant <edurrantatbigpond dot net dot au>
Subject: Re: [os2genau] CD Audio playing problem

I think this reply was meant for Leigh not I,

Cheers,
Ed.

Gavin Miller wrote:
> 
> Hi Ed,
> 
> Try downloading the driver again if it keeps locking up at the end stages.  Sometimes the files can be
> corrupted just enough to do that sort of thing by noise in the lines or whatever.  I've had to do that once or
> twice.
> 
> Cheers.
> 
> ---------------------------------------------------------------------------------------
> To Subscribe/Unsubscribe please go to http://www.os2site.com/list/
> ================================================

3================================================

From: "Robert Traynor  (BobT)" <rtraynoratoptushome dot com dot au>
Date: Sat, 31 Mar 2001 17:33:57 +1000 (EST)
Subject: Re: [os2genau] CD Audio playing problem

Are there any other devices that share the same irq the sblive uses?
If so, ensure that the Sblive has its own IRQ.

In my system, I have manually assigned the SBLive to IRQ 5.

Also, you must disable the PnP OS in your BIOS. The sblive driver depends
on the BIOS configuring the resources for the card. (assigning irq & io ports)
Plug & Play OS =YES   Change to =NO.


Another SBLive user reported recently:-
"I had to load the USB Drivers for Warp and the sb live works fine. 
It will be a problem with the IRQ sharing, please check
which other device shares the soundblaster IRQ."

Other Known problemsfrom the readme.txt file:-
- Crash in PMMERGE when installing the driver on a system that uses the Scitech
  display drivers. 
  Workaround: move the first minstall window (which asks you to select the sb
  driver) almost completely outside of the screen and press enter.

Otherwise you might subscribe to the SBLive egroups site
"sbliveos2ategroups dot com" and post your problem.

Hope this helps,
BobT.



On Fri, 30 Mar 2001 20:41:47 +0830, Leigh Bunting wrote:

>Ed Durrant wrote:
>
>> Sounds like a text book driver issue to me. (Driver incompatible with MMOS2).
>
>I have to admit that installing the driver did lock up in the final stages, so maybe
>it hasn't properly installed - but uninstalling and re-installing causes the same
>lockup. However, I would get a message that the install wasn't complete and get a
>response to retry/continue/cancel. Selecting continue would carry through OK. So maybe
>it gives the appearance of having installed properly.
>
>The entries in the MMPM2.ini file seem to be correct though. I'll uninstall and give
>it another bash.
>--
>Leigh Bunting
>Colonel Light Gardens
>South Australia
>Find out more about Col. Light Gdns. here -
>http://www.cobweb dot com dot au/~pknight/clghs/
>
>
>---------------------------------------------------------------------------------------
>To Subscribe/Unsubscribe please go to http://www.os2site.com/list/
>================================================



















   ,-._|\       Robert Traynor        (BobT)
 /  Oz  \      email            rtraynoratnetstra dot com dot au
 \_,--.x/ 


END================================================
