    KL(IV)                       5/27/74                       KL(IV)

    NAME
         kl - KL-11 or DL-11 asynchronous interface

    DESCRIPTION
         The  discussion  of typewriter I/O given in tty(IV) applies
         to these devices.

         Since they run at a constant speed, attempts to  change  the
         speed via stty(II) are ignored.

         The  on-line  console typewriter is interfaced using a KL-11
         or DL-11.  By appropriate switch settings during  a  reboot,
         UNIX  will  come  up as a single-user system with I/O on the
         console typewriter.

    FILES
         /dev/tty8 console

    SEE ALSO
         tty(IV), init(VIII)

    BUGS
         Modem control for the DL-11E is not implemented.

                                  - 1 -